### Copy/Monitoring Standards

Use Copy/Monitoring to track changes on linked grids and levels

Do not use C/M to track changes on slabs, walls and columns and MEP fixtures. Refer to Section “Ceiling Plan for Lighting and HVAC Diffuser Layout” for additional information on MEP ceiling coordination.