Appendix A – GIS Data Schema

## Data Schema

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Field Name | Field Alias Name | Field Type | Field Length | Field Domain Name |
| SP\_AFLINE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 30 |  |
| START\_NODE | START\_NODE | String | 40 |  |
| START\_BTM | START\_BTM | Double | 8 |  |
| END\_NODE | END\_NODE | String | 40 |  |
| END\_BTM | END\_BTM | Double | 8 |  |
| STATUS | STATUS | String | 40 |  |
| PIPE\_DIA | PIPE\_DIA | SmallInteger | 2 |  |
| PIPE\_MATRL | PIPE\_MATRL | String | 50 |  |
| FLOW\_TYPE | FLOW\_TYPE | String | 40 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 40 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 40 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| OWNER | OWNER | String | 40 |  |
| LOCATION | LOCATION | String | 100 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| PIPE\_TYPE | PIPE\_TYPE | String | 20 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| START\_TOP | START\_TOP | Double | 8 |  |
| END\_TOP | END\_TOP | Double | 8 |  |
| START\_GL | START\_GL | Double | 8 |  |
| END\_GL | END\_GL | Double | 8 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_AFNODE | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GID | GID | Integer | 4 |  |
| SYM\_NAME | SYM\_NAME | String | 40 |  |
| SYM\_SCALE | SYM\_SCALE | Double | 8 |  |
| SYM\_ANGLE | SYM\_ANGLE | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 30 |  |
| NODE\_TYPE | NODE\_TYPE | String | 30 |  |
| NODE\_GL | NODE\_GL | Double | 8 |  |
| NODE\_BTM | NODE\_BTM | Double | 8 |  |
| STATUS | STATUS | String | 30 |  |
| OWNER | OWNER | String | 30 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 30 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| LOCATION | LOCATION | String | 100 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| NODE\_ID | NODE\_ID | Integer | 4 |  |
| FIELD\_LABEL | FIELD\_LABEL | String | 20 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| WEB\_ID | WEB\_ID | String | 10 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| SP\_AFSTRUCTURE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STRUCTURE\_ID | STRUCTURE\_ID | String | 20 |  |
| STRUCTURE\_TYPE | STRUCTURE\_TYPE | String | 30 |  |
| STRUCTURE\_DESC | STRUCTURE\_DESC | String | 100 |  |
| LAYER | LAYER | String | 20 |  |
| BM\_LAYER | BM\_LAYER | String | 20 |  |
| CATEGORY | CATEGORY | String | 20 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_EL\_DUCT\_LINKS | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| START\_NODE | START\_NODE | Integer | 4 |  |
| END\_NODE | END\_NODE | Integer | 4 |  |
| SF\_LINE\_ID | SF\_LINE\_ID | String | 32 |  |
| SFIA\_TAG | SFIA\_TAG | String | 30 |  |
| SF\_START\_NODE | SF\_START\_NODE | String | 30 |  |
| SF\_START\_TAG | SF\_START\_TAG | String | 30 |  |
| START\_BTM | START\_BTM | Double | 8 |  |
| SF\_END\_NODE | SF\_END\_NODE | String | 30 |  |
| SF\_END\_TAG | SF\_END\_TAG | String | 30 |  |
| END\_BTM | END\_BTM | Double | 8 |  |
| SF\_DIAMETER | SF\_DIAMETER | Double | 8 |  |
| SF\_SPARE\_CONDUITS | SF\_SPARE\_CONDUITS | String | 30 |  |
| SF\_DUCT\_TYPE | SF\_DUCT\_TYPE | String | 30 |  |
| SF\_NO\_OF\_CONDUITS | SF\_NO\_OF\_CONDUITS | String | 30 |  |
| SF\_STATUS | SF\_STATUS | String | 30 |  |
| SF\_CONDITION | SF\_CONDITION | String | 30 |  |
| SF\_CONTRACT\_NO | SF\_CONTRACT\_NO | String | 30 |  |
| SF\_YEAR | SF\_YEAR | String | 30 |  |
| SF\_UPDATE\_NO | SF\_UPDATE\_NO | String | 30 |  |
| SF\_UPDATE\_YEAR | SF\_UPDATE\_YEAR | String | 30 |  |
| GENERAL\_LOCATION | GENERAL\_LOCATION | String | 50 |  |
| SF\_COMMENTS | SF\_COMMENTS | String | 255 |  |
| OLD\_OLD\_GID | OLD\_OLD\_GID | Integer | 4 |  |
| CONDUITS\_TOTAL | CONDUITS\_TOTAL | SmallInteger | 2 |  |
| CONDUITS\_CONFIG | CONDUITS\_CONFIG | String | 30 |  |
| CONDUITS\_USED | CONDUITS\_USED | SmallInteger | 2 |  |
| CONDUITS\_SPARE | CONDUITS\_SPARE | SmallInteger | 2 |  |
| DUCT\_DETL\_STATUS | DUCT\_DETL\_STATUS | String | 10 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| LAYER | LAYER | String | 20 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| START\_TOP | START\_TOP | Double | 8 |  |
| END\_TOP | END\_TOP | Double | 8 |  |
| DUCT\_HT | DUCT\_HT | Double | 8 |  |
| DUCT\_WIDTH | DUCT\_WIDTH | Double | 8 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_EL\_DUCT\_NODES | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| SYM\_NAME | SYM\_NAME | String | 40 |  |
| SYM\_SCALE | SYM\_SCALE | Double | 8 |  |
| SYM\_ANGLE | SYM\_ANGLE | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| NODE\_ID | NODE\_ID | Integer | 4 |  |
| NODE\_TYPE | NODE\_TYPE | String | 20 |  |
| NODE\_DESC | NODE\_DESC | String | 20 |  |
| NODE\_REF | NODE\_REF | String | 40 |  |
| LINK\_ID | LINK\_ID | String | 40 |  |
| SFO\_NUMBER | SFO\_NUMBER | String | 50 |  |
| CONTRACT | CONTRACT | String | 50 |  |
| YR\_INSTALLED | YR\_INSTALLED | String | 50 |  |
| ACTIVE | ACTIVE | String | 1 |  |
| LOCATION | LOCATION | String | 50 |  |
| PLAN | PLAN | String | 50 |  |
| DETAIL | DETAIL | String | 50 |  |
| FORMER\_NUMBER | FORMER\_NUMBER | String | 50 |  |
| BUTTERFLY\_DWG | BUTTERFLY\_DWG | String | 1 |  |
| MH\_FOLDER\_LINK | MH\_FOLDER\_LINK | String | 250 |  |
| REMARKS | REMARKS | String | 50 |  |
| SFO\_SYM\_NAME | SFO\_SYM\_NAME | String | 40 |  |
| DATA\_ISSUES | DATA\_ISSUES | String | 60 |  |
| PDMH\_NODE\_ID | PDMH\_NODE\_ID | String | 32 |  |
| PDMH\_NODE\_TYPE | PDMH\_NODE\_TYPE | String | 30 |  |
| PDMH\_LIB\_REF | PDMH\_LIB\_REF | String | 30 |  |
| PDMH\_FORMER\_SFIA\_TAG | PDMH\_FORMER\_SFIA\_TAG | String | 30 |  |
| NODE\_GL | NODE\_GL | Double | 8 |  |
| NODE\_INV | NODE\_INV | Double | 8 |  |
| PDMH\_STATUS | PDMH\_STATUS | String | 30 |  |
| PDMH\_DIMENSIONS | PDMH\_DIMENSIONS | String | 30 |  |
| PDMH\_NECK\_HT | PDMH\_NECK\_HT | Double | 8 |  |
| PDMH\_DETAIL\_DWG | PDMH\_DETAIL\_DWG | String | 30 |  |
| PDMH\_PLAN\_DWG | PDMH\_PLAN\_DWG | String | 30 |  |
| PDMH\_CONTRACT\_NO | PDMH\_CONTRACT\_NO | String | 30 |  |
| PDMH\_UPDATE\_NO | PDMH\_UPDATE\_NO | String | 50 |  |
| PDMH\_UPDATE\_YEAR | PDMH\_UPDATE\_YEAR | String | 50 |  |
| PDMH\_GENERAL\_LOCATION | PDMH\_GENERAL\_LOCATION | String | 30 |  |
| PDMH\_COMMENTS | PDMH\_COMMENTS | String | 255 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| LAYER | LAYER | String | 20 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| NODE\_GL\_TEMP | NODE\_GL\_TEMP | Double | 8 |  |
| NODE\_INV\_TEMP | NODE\_INV\_TEMP | Double | 8 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| PDMH\_YEAR | PDMH\_YEAR | Double | 8 |  |
| WEB\_ID | WEB\_ID | String | 10 |  |
| SP\_EL\_STRUCTURS\_LN | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 20 |  |
| STRUCTURE\_DESC | STRUCTURE\_DESC | String | 100 |  |
| BM\_LAYER | BM\_LAYER | String | 20 |  |
| STRUCTURE\_ID | STRUCTURE\_ID | String | 10 |  |
| STRUCTURE\_TYPE | STRUCTURE\_TYPE | String | 20 |  |
| CATEGORY | CATEGORY | String | 20 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_IWLINE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 40 |  |
| STATUS | STATUS | String | 40 |  |
| OWNER | OWNER | String | 40 |  |
| START\_NODE | START\_NODE | String | 40 |  |
| END\_NODE | END\_NODE | String | 40 |  |
| START\_INVELEV | START\_INVELEV | Double | 8 |  |
| END\_INVELEV | END\_INVELEV | Double | 8 |  |
| PIPE\_MATRL | PIPE\_MATRL | String | 50 |  |
| PIPE\_DIA | PIPE\_DIA | SmallInteger | 2 |  |
| FLOW\_TYPE | FLOW\_TYPE | String | 40 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 40 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 40 |  |
| LOCATION | LOCATION | String | 100 |  |
| PIPE\_TYPE | PIPE\_TYPE | String | 20 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| START\_COVELEV | START\_COVELEV | Double | 8 |  |
| END\_COVELEV | END\_COVELEV | Double | 8 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_IWNODE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| SYM\_NAME | SYM\_NAME | String | 40 |  |
| SYM\_SCALE | SYM\_SCALE | Double | 8 |  |
| SYM\_ANGLE | SYM\_ANGLE | Double | 8 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 20 |  |
| NODE\_TYPE | NODE\_TYPE | String | 30 |  |
| STATUS | STATUS | String | 40 |  |
| NODE\_COVELEV | NODE\_COVELEV | Double | 8 |  |
| NODE\_INV | NODE\_INV | Double | 8 |  |
| FLOW\_TYPE | FLOW\_TYPE | String | 40 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 40 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 40 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| OWNER | OWNER | String | 40 |  |
| LOCATION | LOCATION | String | 100 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| PUMPSTA\_NAME | PUMPSTA\_NAME | String | 20 |  |
| NODE\_ID | NODE\_ID | Integer | 4 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| NODE\_DEPTH | NODE\_DEPTH | Double | 8 |  |
| WEB\_ID | WEB\_ID | String | 10 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| SP\_IWSTRUCTURE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STRUCTURE\_ID | STRUCTURE\_ID | String | 20 |  |
| STRUCTURE\_TYPE | STRUCTURE\_TYPE | String | 30 |  |
| STRUCTURE\_DESC | STRUCTURE\_DESC | String | 100 |  |
| LAYER | LAYER | String | 20 |  |
| BM\_LAYER | BM\_LAYER | String | 20 |  |
| CATEGORY | CATEGORY | String | 20 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_NGLINE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 20 |  |
| STATUS | STATUS | String | 40 |  |
| OWNER | OWNER | String | 40 |  |
| START\_NODE | START\_NODE | String | 40 |  |
| END\_NODE | END\_NODE | String | 40 |  |
| START\_TOP | START\_TOP | Double | 8 |  |
| END\_TOP | END\_TOP | Double | 8 |  |
| PIPE\_MATRL | PIPE\_MATRL | String | 50 |  |
| PIPE\_DIA | PIPE\_DIA | SmallInteger | 2 |  |
| FLOW\_TYPE | FLOW\_TYPE | String | 40 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 40 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 40 |  |
| LOCATION | LOCATION | String | 100 |  |
| PIPE\_TYPE | PIPE\_TYPE | String | 20 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| START\_GL | START\_GL | Double | 8 |  |
| END\_GL | END\_GL | Double | 8 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_NGNODE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| SYM\_NAME | SYM\_NAME | String | 40 |  |
| SYM\_SCALE | SYM\_SCALE | Double | 8 |  |
| SYM\_ANGLE | SYM\_ANGLE | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 20 |  |
| NODE\_TYPE | NODE\_TYPE | String | 40 |  |
| STATUS | STATUS | String | 40 |  |
| NODE\_GL | NODE\_GL | Double | 8 |  |
| NODE\_BTM | NODE\_BTM | Double | 8 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 40 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 40 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| OWNER | OWNER | String | 40 |  |
| LOCATION | LOCATION | String | 100 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| NODE\_ID | NODE\_ID | Integer | 4 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| WEB\_ID | WEB\_ID | String | 10 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| SP\_NGSTRUCTURE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STRUCTURE\_ID | STRUCTURE\_ID | String | 20 |  |
| STRUCTURE\_TYPE | STRUCTURE\_TYPE | String | 30 |  |
| STRUCTURE\_DESC | STRUCTURE\_DESC | String | 100 |  |
| LAYER | LAYER | String | 20 |  |
| BM\_LAYER | BM\_LAYER | String | 20 |  |
| CATEGORY | CATEGORY | String | 20 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SEWGPIPE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| PIPE\_ID | PIPE\_ID | Integer | 4 |  |
| PIPE\_GRADIENT | PIPE\_GRADIENT | Double | 8 |  |
| PIPE\_DIA | PIPE\_DIA | Single | 4 |  |
| PIPE\_TYPE | PIPE\_TYPE | String | 30 |  |
| PIPE\_MATRL | PIPE\_MATRL | String | 50 |  |
| START\_NODE | START\_NODE | Integer | 4 |  |
| END\_NODE | END\_NODE | Integer | 4 |  |
| START\_COVELEV | START\_COVELEV | Double | 8 |  |
| END\_COVELEV | END\_COVELEV | Double | 8 |  |
| START\_INVELEV | START\_INVELEV | Double | 8 |  |
| END\_INVELEV | END\_INVELEV | Double | 8 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 40 |  |
| STATUS | STATUS | String | 10 |  |
| FLOW\_TYPE | FLOW\_TYPE | String | 10 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 20 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| LOCATION | LOCATION | String | 100 |  |
| OWNER | OWNER | String | 50 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SEWNODE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| NODE\_ID | NODE\_ID | Integer | 4 |  |
| NODE\_TYPE | NODE\_TYPE | String | 20 |  |
| NODE\_DEPTH | NODE\_DEPTH | Double | 8 |  |
| NODE\_COVELEV | NODE\_COVELEV | Double | 8 |  |
| NODE\_REF | NODE\_REF | String | 20 |  |
| SYM\_NAME | SYM\_NAME | String | 40 |  |
| SYM\_SCALE | SYM\_SCALE | Double | 8 |  |
| SYM\_ANGLE | SYM\_ANGLE | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STATUS | STATUS | String | 10 |  |
| NODE\_INV | NODE\_INV | Double | 8 |  |
| FLOW\_TYPE | FLOW\_TYPE | String | 10 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 20 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| LOCATION | LOCATION | String | 100 |  |
| OWNER | OWNER | String | 50 |  |
| LAYER | LAYER | String | 40 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| PUMPSTA\_NAME | PUMPSTA\_NAME | String | 20 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| WEB\_ID | WEB\_ID | String | 10 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| SP\_SEWRPIPE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| PIPE\_ID | PIPE\_ID | Integer | 4 |  |
| PIPE\_GRADIENT | PIPE\_GRADIENT | Double | 8 |  |
| PIPE\_DIA | PIPE\_DIA | Single | 4 |  |
| PIPE\_TYPE | PIPE\_TYPE | String | 30 |  |
| PIPE\_MATRL | PIPE\_MATRL | String | 50 |  |
| START\_NODE | START\_NODE | Integer | 4 |  |
| END\_NODE | END\_NODE | Integer | 4 |  |
| START\_COVELEV | START\_COVELEV | Double | 8 |  |
| END\_COVELEV | END\_COVELEV | Double | 8 |  |
| START\_INVELEV | START\_INVELEV | Double | 8 |  |
| END\_INVELEV | END\_INVELEV | Double | 8 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 40 |  |
| STATUS | STATUS | String | 10 |  |
| FLOW\_TYPE | FLOW\_TYPE | String | 10 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 20 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| LOCATION | LOCATION | String | 100 |  |
| OWNER | OWNER | String | 50 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SEWSTRUCTURE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STRUCTURE\_ID | STRUCTURE\_ID | String | 20 |  |
| STRUCTURE\_TYPE | STRUCTURE\_TYPE | String | 30 |  |
| STRUCTURE\_DESC | STRUCTURE\_DESC | String | 100 |  |
| LAYER | LAYER | String | 20 |  |
| BM\_LAYER | BM\_LAYER | String | 20 |  |
| CATEGORY | CATEGORY | String | 20 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SFO\_TEDUCT | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| SFO\_LAYER | SFO\_LAYER | String | 50 |  |
| SFO\_DUCT\_ID | SFO\_DUCT\_ID | String | 50 |  |
| LAYER | LAYER | String | 20 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SFO\_TECU\_LINES | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LINE\_MATERIAL | LINE\_MATERIAL | String | 35 |  |
| LAYER | LAYER | String | 20 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SFO\_TEFI\_LINES | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 20 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SFO\_TENODE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| SYM\_NAME | SYM\_NAME | String | 40 |  |
| SYM\_SCALE | SYM\_SCALE | Double | 8 |  |
| SYM\_ANGLE | SYM\_ANGLE | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| SFO\_LAYER | SFO\_LAYER | String | 20 |  |
| SFO\_NODE\_ID | SFO\_NODE\_ID | String | 50 |  |
| NODE\_TYPE | NODE\_TYPE | String | 10 |  |
| LIB\_REF | LIB\_REF | String | 10 |  |
| STATUS | STATUS | String | 10 |  |
| NODE\_GL | NODE\_GL | Double | 8 |  |
| NODE\_INV | NODE\_INV | Double | 8 |  |
| NODE\_SIZE | NODE\_SIZE | String | 50 |  |
| LADDER | LADDER | String | 20 |  |
| WIDTH | WIDTH | Double | 8 |  |
| LENGTH | LENGTH | Double | 8 |  |
| CEILING\_HEIGHT | CEILING\_HEIGHT | Double | 8 |  |
| NECK\_HEIGHT | NECK\_HEIGHT | Double | 8 |  |
| COVER\_SIZE | COVER\_SIZE | Double | 8 |  |
| COVER\_LABEL | COVER\_LABEL | String | 20 |  |
| INSPECTION | INSPECTION | String | 4 |  |
| BUTTERFLY | BUTTERFLY | String | 20 |  |
| INSTALL\_CONT | INSTALL\_CONT | String | 20 |  |
| INSTALL\_YEAR | INSTALL\_YEAR | String | 20 |  |
| UPDATE\_CONT | UPDATE\_CONT | String | 20 |  |
| UPDATE\_YEAR | UPDATE\_YEAR | String | 20 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| LOCATION | LOCATION | String | 50 |  |
| CONDITION | CONDITION | String | 20 |  |
| DEBRIS | DEBRIS | String | 20 |  |
| OWNER | OWNER | String | 50 |  |
| SFO\_COMMENT | SFO\_COMMENT | String | 255 |  |
| LAYER | LAYER | String | 20 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| WEB\_ID | WEB\_ID | String | 12 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| SP\_SFO\_TESTRUCTURE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| SFO\_LAYER | SFO\_LAYER | String | 20 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SWNODE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| NODE\_ID | NODE\_ID | Integer | 4 |  |
| NODE\_TYPE | NODE\_TYPE | String | 30 |  |
| NODE\_DEPTH | NODE\_DEPTH | Double | 8 |  |
| NODE\_GL | NODE\_GL | Double | 8 |  |
| NODE\_SIZE1 | NODE\_SIZE1 | Double | 8 |  |
| NODE\_SIZE2 | NODE\_SIZE2 | Double | 8 |  |
| SYM\_NAME | SYM\_NAME | String | 40 |  |
| SYM\_SCALE | SYM\_SCALE | Double | 8 |  |
| SYM\_ANGLE | SYM\_ANGLE | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STATUS | STATUS | String | 10 |  |
| NODE\_INV | NODE\_INV | Double | 8 |  |
| FLOW\_TYPE | FLOW\_TYPE | String | 10 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 20 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| LOCATION | LOCATION | String | 100 |  |
| LAYER | LAYER | String | 50 |  |
| OWNER | OWNER | String | 50 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| PUMPSTA\_NAME | PUMPSTA\_NAME | String | 20 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| WEB\_ID | WEB\_ID | String | 10 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| SP\_SWCULVERT | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| CLVT\_GRADIENT | CLVT\_GRADIENT | Double | 8 |  |
| CLVT\_WIDTH | CLVT\_WIDTH | Single | 4 |  |
| CLVT\_DEPTH | CLVT\_DEPTH | Single | 4 |  |
| CLVT\_TYPE | CLVT\_TYPE | String | 20 |  |
| CLVT\_MATRL | CLVT\_MATRL | String | 20 |  |
| START\_NODE | START\_NODE | Integer | 4 |  |
| END\_NODE | END\_NODE | Integer | 4 |  |
| START\_GL | START\_GL | Double | 8 |  |
| END\_GL | END\_GL | Double | 8 |  |
| START\_IL | START\_IL | Double | 8 |  |
| END\_IL | END\_IL | Double | 8 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STATUS | STATUS | String | 10 |  |
| FLOW\_TYPE | FLOW\_TYPE | String | 20 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 20 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | String | 20 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| LOCATION | LOCATION | String | 50 |  |
| OWNER | OWNER | String | 50 |  |
| OLD\_LINE\_ID | OLD\_LINE\_ID | String | 50 |  |
| LAYER | LAYER | String | 50 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SWPIPE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| PIPE\_GRADIENT | PIPE\_GRADIENT | Double | 8 |  |
| PIPE\_DIA | PIPE\_DIA | Single | 4 |  |
| PIPE\_TYPE | PIPE\_TYPE | String | 20 |  |
| PIPE\_MATRL | PIPE\_MATRL | String | 50 |  |
| START\_NODE | START\_NODE | Integer | 4 |  |
| END\_NODE | END\_NODE | Integer | 4 |  |
| START\_GL | START\_GL | Double | 8 |  |
| END\_GL | END\_GL | Double | 8 |  |
| START\_IL | START\_IL | Double | 8 |  |
| END\_IL | END\_IL | Double | 8 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STATUS | STATUS | String | 10 |  |
| FLOW\_TYPE | FLOW\_TYPE | String | 20 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 20 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| LOCATION | LOCATION | String | 100 |  |
| OWNER | OWNER | String | 50 |  |
| LAYER | LAYER | String | 50 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| PIPE\_ID | PIPE\_ID | Integer | 4 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SWSTRUCTURE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STRUCTURE\_ID | STRUCTURE\_ID | String | 20 |  |
| STRUCTURE\_TYPE | STRUCTURE\_TYPE | String | 30 |  |
| STRUCTURE\_DESC | STRUCTURE\_DESC | String | 100 |  |
| LAYER | LAYER | String | 20 |  |
| BM\_LAYER | BM\_LAYER | String | 20 |  |
| CATEGORY | CATEGORY | String | 20 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_SWCHANNEL | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| CHNL\_GRADIENT | CHNL\_GRADIENT | Double | 8 |  |
| CHNL\_BWIDTH | CHNL\_BWIDTH | Single | 4 |  |
| CHNL\_TWIDTH | CHNL\_TWIDTH | Single | 4 |  |
| CHNL\_DEPTH | CHNL\_DEPTH | Single | 4 |  |
| CHNL\_TYPE | CHNL\_TYPE | String | 20 |  |
| CHNL\_MATRL | CHNL\_MATRL | String | 20 |  |
| START\_NODE | START\_NODE | Integer | 4 |  |
| END\_NODE | END\_NODE | Integer | 4 |  |
| START\_GL | START\_GL | Double | 8 |  |
| END\_GL | END\_GL | Double | 8 |  |
| START\_IL | START\_IL | Double | 8 |  |
| END\_IL | END\_IL | Double | 8 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| LAYER | LAYER | String | 50 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_WATNODE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| NODE\_ID | NODE\_ID | Integer | 4 |  |
| NODE\_TYPE | NODE\_TYPE | String | 30 |  |
| NODE\_ELEV | NODE\_ELEV | Double | 8 |  |
| NODE\_REF | NODE\_REF | String | 20 |  |
| WAT\_CATEGORY | WAT\_CATEGORY | String | 20 |  |
| SYM\_NAME | SYM\_NAME | String | 40 |  |
| SYM\_SCALE | SYM\_SCALE | Double | 8 |  |
| SYM\_ANGLE | SYM\_ANGLE | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STATUS | STATUS | String | 30 |  |
| NODE\_BTM | NODE\_BTM | Double | 8 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 30 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| LOCATION | LOCATION | String | 100 |  |
| OWNER | OWNER | String | 50 |  |
| LAYER | LAYER | String | 50 |  |
| FIELD\_TAG | FIELD\_TAG | String | 20 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| HYDRANT\_ID | HYDRANT\_ID | String | 10 |  |
| HYDRANT\_VLV | HYDRANT\_VLV | String | 2 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| EXERCISED\_DATE | EXERCISED\_DATE | String | 4 |  |
| EXERCISED\_BY | EXERCISED\_BY | String | 40 |  |
| WEB\_ID | WEB\_ID | String | 10 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| SP\_WATPIPE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| PIPE\_ID | PIPE\_ID | Integer | 4 |  |
| PIPE\_DIA | PIPE\_DIA | Single | 4 |  |
| PIPE\_TYPE | PIPE\_TYPE | String | 20 |  |
| PIPE\_MATRL | PIPE\_MATRL | String | 50 |  |
| START\_NODE | START\_NODE | Integer | 4 |  |
| END\_NODE | END\_NODE | Integer | 4 |  |
| WAT\_CATEGORY | WAT\_CATEGORY | String | 20 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 400 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| START\_BTM | START\_BTM | Double | 8 |  |
| END\_BTM | END\_BTM | Double | 8 |  |
| STATUS | STATUS | String | 30 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 30 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | Integer | 4 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| LOCATION | LOCATION | String | 100 |  |
| LAYER | LAYER | String | 50 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| OWNER | OWNER | String | 20 |  |
| SPATIAL\_DATE | SPATIAL\_DATE | Date | 8 |  |
| FAA\_SUE | FAA\_SUE | String | 5 |  |
| START\_GL | START\_GL | Double | 8 |  |
| END\_GL | END\_GL | Double | 8 |  |
| END\_TOP | END\_TOP | Double | 8 |  |
| START\_TOP | START\_TOP | Double | 8 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| SP\_WATSTRUCTURE | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| STRUCTURE\_ID | STRUCTURE\_ID | String | 20 |  |
| STRUCTURE\_TYPE | STRUCTURE\_TYPE | String | 30 |  |
| STRUCTURE\_DESC | STRUCTURE\_DESC | String | 100 |  |
| LAYER | LAYER | String | 20 |  |
| BM\_LAYER | BM\_LAYER | String | 20 |  |
| CATEGORY | CATEGORY | String | 20 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| GBME\_11x17\_ANNO | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FEATUREID | FEATUREID | Integer | 4 |  |
| ZORDER | ZORDER | Integer | 4 |  |
| ANNOTATIONCLASSID | ANNOTATIONCLASSID | Integer | 4 |  |
| ELEMENT | ELEMENT | Blob | 0 |  |
| SYMBOLID | SYMBOLID | Integer | 4 |  |
| STATUS | STATUS | SmallInteger | 2 | AnnotationStatus |
| TEXTSTRING | TEXTSTRING | String | 255 |  |
| FONTNAME | FONTNAME | String | 255 |  |
| FONTSIZE | FONTSIZE | Double | 8 |  |
| BOLD | BOLD | SmallInteger | 2 | BooleanSymbolValue |
| ITALIC | ITALIC | SmallInteger | 2 | BooleanSymbolValue |
| UNDERLINE | UNDERLINE | SmallInteger | 2 | BooleanSymbolValue |
| VERTICALALIGNMENT | VERTICALALIGNMENT | SmallInteger | 2 | VerticalAlignment |
| HORIZONTALALIGNMENT | HORIZONTALALIGNMENT | SmallInteger | 2 | HorizontalAlignment |
| XOFFSET | XOFFSET | Double | 8 |  |
| YOFFSET | YOFFSET | Double | 8 |  |
| ANGLE | ANGLE | Double | 8 |  |
| FONTLEADING | FONTLEADING | Double | 8 |  |
| WORDSPACING | WORDSPACING | Double | 8 |  |
| CHARACTERWIDTH | CHARACTERWIDTH | Double | 8 |  |
| CHARACTERSPACING | CHARACTERSPACING | Double | 8 |  |
| FLIPANGLE | FLIPANGLE | Double | 8 |  |
| OVERRIDE | OVERRIDE | Integer | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_17x22\_ANNO | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FEATUREID | FEATUREID | Integer | 4 |  |
| ZORDER | ZORDER | Integer | 4 |  |
| ANNOTATIONCLASSID | ANNOTATIONCLASSID | Integer | 4 |  |
| ELEMENT | ELEMENT | Blob | 0 |  |
| SYMBOLID | SYMBOLID | Integer | 4 |  |
| STATUS | STATUS | SmallInteger | 2 | AnnotationStatus |
| TEXTSTRING | TEXTSTRING | String | 255 |  |
| FONTNAME | FONTNAME | String | 255 |  |
| FONTSIZE | FONTSIZE | Double | 8 |  |
| BOLD | BOLD | SmallInteger | 2 | BooleanSymbolValue |
| ITALIC | ITALIC | SmallInteger | 2 | BooleanSymbolValue |
| UNDERLINE | UNDERLINE | SmallInteger | 2 | BooleanSymbolValue |
| VERTICALALIGNMENT | VERTICALALIGNMENT | SmallInteger | 2 | VerticalAlignment |
| HORIZONTALALIGNMENT | HORIZONTALALIGNMENT | SmallInteger | 2 | HorizontalAlignment |
| XOFFSET | XOFFSET | Double | 8 |  |
| YOFFSET | YOFFSET | Double | 8 |  |
| ANGLE | ANGLE | Double | 8 |  |
| FONTLEADING | FONTLEADING | Double | 8 |  |
| WORDSPACING | WORDSPACING | Double | 8 |  |
| CHARACTERWIDTH | CHARACTERWIDTH | Double | 8 |  |
| CHARACTERSPACING | CHARACTERSPACING | Double | 8 |  |
| FLIPANGLE | FLIPANGLE | Double | 8 |  |
| OVERRIDE | OVERRIDE | Integer | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_22x34\_ANNO | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FEATUREID | FEATUREID | Integer | 4 |  |
| ZORDER | ZORDER | Integer | 4 |  |
| ANNOTATIONCLASSID | ANNOTATIONCLASSID | Integer | 4 |  |
| ELEMENT | ELEMENT | Blob | 0 |  |
| SYMBOLID | SYMBOLID | Integer | 4 |  |
| STATUS | STATUS | SmallInteger | 2 | AnnotationStatus |
| TEXTSTRING | TEXTSTRING | String | 255 |  |
| FONTNAME | FONTNAME | String | 255 |  |
| FONTSIZE | FONTSIZE | Double | 8 |  |
| BOLD | BOLD | SmallInteger | 2 | BooleanSymbolValue |
| ITALIC | ITALIC | SmallInteger | 2 | BooleanSymbolValue |
| UNDERLINE | UNDERLINE | SmallInteger | 2 | BooleanSymbolValue |
| VERTICALALIGNMENT | VERTICALALIGNMENT | SmallInteger | 2 | VerticalAlignment |
| HORIZONTALALIGNMENT | HORIZONTALALIGNMENT | SmallInteger | 2 | HorizontalAlignment |
| XOFFSET | XOFFSET | Double | 8 |  |
| YOFFSET | YOFFSET | Double | 8 |  |
| ANGLE | ANGLE | Double | 8 |  |
| FONTLEADING | FONTLEADING | Double | 8 |  |
| WORDSPACING | WORDSPACING | Double | 8 |  |
| CHARACTERWIDTH | CHARACTERWIDTH | Double | 8 |  |
| CHARACTERSPACING | CHARACTERSPACING | Double | 8 |  |
| FLIPANGLE | FLIPANGLE | Double | 8 |  |
| OVERRIDE | OVERRIDE | Integer | 4 |  |
| TYPE | TYPE | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_34x44\_ANNO | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FEATUREID | FEATUREID | Integer | 4 |  |
| ZORDER | ZORDER | Integer | 4 |  |
| ANNOTATIONCLASSID | ANNOTATIONCLASSID | Integer | 4 |  |
| ELEMENT | ELEMENT | Blob | 0 |  |
| SYMBOLID | SYMBOLID | Integer | 4 |  |
| STATUS | STATUS | SmallInteger | 2 | AnnotationStatus |
| TEXTSTRING | TEXTSTRING | String | 255 |  |
| FONTNAME | FONTNAME | String | 255 |  |
| FONTSIZE | FONTSIZE | Double | 8 |  |
| BOLD | BOLD | SmallInteger | 2 | BooleanSymbolValue |
| ITALIC | ITALIC | SmallInteger | 2 | BooleanSymbolValue |
| UNDERLINE | UNDERLINE | SmallInteger | 2 | BooleanSymbolValue |
| VERTICALALIGNMENT | VERTICALALIGNMENT | SmallInteger | 2 | VerticalAlignment |
| HORIZONTALALIGNMENT | HORIZONTALALIGNMENT | SmallInteger | 2 | HorizontalAlignment |
| XOFFSET | XOFFSET | Double | 8 |  |
| YOFFSET | YOFFSET | Double | 8 |  |
| ANGLE | ANGLE | Double | 8 |  |
| FONTLEADING | FONTLEADING | Double | 8 |  |
| WORDSPACING | WORDSPACING | Double | 8 |  |
| CHARACTERWIDTH | CHARACTERWIDTH | Double | 8 |  |
| CHARACTERSPACING | CHARACTERSPACING | Double | 8 |  |
| FLIPANGLE | FLIPANGLE | Double | 8 |  |
| OVERRIDE | OVERRIDE | Integer | 4 |  |
| ANNO\_CLASS | ANNO\_CLASS | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_34x44\_ANNO\_MASTER | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FEATUREID | FEATUREID | Integer | 4 |  |
| ZORDER | ZORDER | Integer | 4 |  |
| ANNOTATIONCLASSID | ANNOTATIONCLASSID | Integer | 4 |  |
| SYMBOLID | SYMBOLID | Integer | 4 |  |
| STATUS | STATUS | SmallInteger | 2 | AnnotationStatus |
| TEXTSTRING | TEXTSTRING | String | 255 |  |
| FONTNAME | FONTNAME | String | 255 |  |
| FONTSIZE | FONTSIZE | Double | 8 |  |
| BOLD | BOLD | SmallInteger | 2 | BooleanSymbolValue |
| ITALIC | ITALIC | SmallInteger | 2 | BooleanSymbolValue |
| UNDERLINE | UNDERLINE | SmallInteger | 2 | BooleanSymbolValue |
| VERTICALALIGNMENT | VERTICALALIGNMENT | SmallInteger | 2 | VerticalAlignment |
| HORIZONTALALIGNMENT | HORIZONTALALIGNMENT | SmallInteger | 2 | HorizontalAlignment |
| XOFFSET | XOFFSET | Double | 8 |  |
| YOFFSET | YOFFSET | Double | 8 |  |
| ANGLE | ANGLE | Double | 8 |  |
| FONTLEADING | FONTLEADING | Double | 8 |  |
| WORDSPACING | WORDSPACING | Double | 8 |  |
| CHARACTERWIDTH | CHARACTERWIDTH | Double | 8 |  |
| CHARACTERSPACING | CHARACTERSPACING | Double | 8 |  |
| FLIPANGLE | FLIPANGLE | Double | 8 |  |
| OVERRIDE | OVERRIDE | Integer | 4 |  |
| ANNO\_CLASS | ANNO\_CLASS | String | 50 |  |
| ORIG\_FID | ORIG\_FID | Integer | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| ROTATION | ROTATION | SmallInteger | 2 |  |
| CADTYPE | CADTYPE | String | 50 |  |
| TXTVALUE | TXTVALUE | String | 50 |  |
| GBME\_34x44\_STRUCTURE\_OVERUN | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_AIR\_OPERATIONS\_AREA | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| GID | GID | Integer | 4 |  |
| NAME | NAME | String | 50 |  |
| DESCRIP | DESCRIP | String | 254 |  |
| STATUS | STATUS | String | 20 |  |
| ALTERNATIV | ALTERNATIV | Integer | 4 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| USERFLAG | USERFLAG | String | 254 |  |
| CADDLAYERN | CADDLAYERN | String | 40 |  |
| CADDLAYERD | CADDLAYERD | String | 50 |  |
| CADDCOLOR | CADDCOLOR | Integer | 4 |  |
| DATEDATAAC | DATEDATAAC | Date | 8 |  |
| DATASOURCE | DATASOURCE | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE\_LENG | Shape\_Leng | Double | 8 |  |
| MODIFIED | Modified | String | 254 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| CALC\_AREA | CALC\_AREA | Double | 8 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_AIRCRAFT\_GATE\_STAND | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| GATESTTYPE | Gate Stand Type | String | 16 | CodeGateStandType |
| DESCRIP | Description | String | 255 |  |
| WINGSPAN | Wingspan | Integer | 4 |  |
| LENGTH | Length | Integer | 4 |  |
| WIDTH | Width | Integer | 4 |  |
| PAVEMENTCL | Pavement Classification Number | String | 10 |  |
| JETWAYAVAI | Jetway Availability | String | 1 | CodeBoolean |
| TOWINGAVAI | Towing Availability | String | 1 | CodeBoolean |
| DOCKINGAVA | Docking Availability | String | 1 | CodeBoolean |
| GROUNDPOWE | Ground Power Availability | String | 1 | CodeBoolean |
| SURFACET | Surface Type | String | 16 | CodeSurfaceType |
| SURFACEC | Surface Condition | String | 16 | CodeSurfaceCondition |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| COMMENTS | Comments | String | 150 |  |
| USERFLAG | User Flag | String | 254 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | Shape | Geometry | 0 |  |
| GBME\_AIRPORT\_BOUNDARY | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| FAASITENR | Faa Site Number | String | 8 |  |
| DESCRIP | Description | String | 255 |  |
| FAALOCID | Faa Location Id | String | 4 |  |
| IATACODE | IATA Code | String | 4 |  |
| ICAOCODE | ICAO Code | String | 4 |  |
| AIRPORTFAC | Airport Facility Type | String | 16 |  |
| OPERATIO | Operations Type | String | 16 |  |
| OWNER | Owner | String | 16 | CodeOwner |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| COMMENTS | Comments | String | 150 |  |
| USERFLAG | User Flag | String | 254 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | Shape | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_ANNO\_CAD | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FEATUREID | FEATUREID | Integer | 4 |  |
| ZORDER | ZORDER | Integer | 4 |  |
| ANNOTATIONCLASSID | ANNOTATIONCLASSID | Integer | 4 |  |
| ELEMENT | ELEMENT | Blob | 0 |  |
| SYMBOLID | SYMBOLID | Integer | 4 |  |
| STATUS | STATUS | SmallInteger | 2 | AnnotationStatus |
| TEXTSTRING | TEXTSTRING | String | 255 |  |
| FONTNAME | FONTNAME | String | 255 |  |
| FONTSIZE | FONTSIZE | Double | 8 |  |
| BOLD | BOLD | SmallInteger | 2 | BooleanSymbolValue |
| ITALIC | ITALIC | SmallInteger | 2 | BooleanSymbolValue |
| UNDERLINE | UNDERLINE | SmallInteger | 2 | BooleanSymbolValue |
| VERTICALALIGNMENT | VERTICALALIGNMENT | SmallInteger | 2 | VerticalAlignment |
| HORIZONTALALIGNMENT | HORIZONTALALIGNMENT | SmallInteger | 2 | HorizontalAlignment |
| XOFFSET | XOFFSET | Double | 8 |  |
| YOFFSET | YOFFSET | Double | 8 |  |
| ANGLE | ANGLE | Double | 8 |  |
| FONTLEADING | FONTLEADING | Double | 8 |  |
| WORDSPACING | WORDSPACING | Double | 8 |  |
| CHARACTERWIDTH | CHARACTERWIDTH | Double | 8 |  |
| CHARACTERSPACING | CHARACTERSPACING | Double | 8 |  |
| FLIPANGLE | FLIPANGLE | Double | 8 |  |
| OVERRIDE | OVERRIDE | Integer | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_ARP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| ENTITY | ENTITY | String | 16 |  |
| LAYER | Layer | String | 255 |  |
| COLOR | Color | SmallInteger | 2 |  |
| LINETYPE | Linetype | String | 255 |  |
| ELEVATION | Elevation | Double | 8 |  |
| LINEWT | LineWt | SmallInteger | 2 |  |
| REFNAME | RefName | String | 255 |  |
| ORIG\_FID | ORIG\_FID | Integer | 4 |  |
| X | X | Double | 8 |  |
| Y | Y | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| GBME\_BASE | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| LAYER | LAYER | String | 254 |  |
| ENTITY | ENTITY | String | 16 |  |
| COLOR | COLOR | Integer | 4 |  |
| LINETYPE | LINETYPE | String | 254 |  |
| ELEVATION | ELEVATION | Double | 8 |  |
| LINEWT | LINEWT | Integer | 4 |  |
| REFNAME | REFNAME | String | 254 |  |
| NAME | NAME | String | 40 |  |
| CATEGORY | CATEGORY | String | 20 |  |
| DESCRIPTION | DESCRIPTION | String | 50 |  |
| LEVEL\_ | LEVEL\_ | Double | 8 |  |
| NOTES | NOTES | String | 100 |  |
| CAD\_LAYER | CAD\_LAYER | String | 100 |  |
| GDS\_ID | GDS\_ID | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_BASE\_FEAT | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| LAYER | LAYER | String | 50 |  |
| LEVEL\_ | LEVEL\_ | Double | 8 |  |
| NAME | NAME | String | 50 |  |
| CATEGORY | CATEGORY | String | 50 |  |
| DESCRIPTION | DESCRIPTION | String | 50 |  |
| NOTES | NOTES | String | 200 |  |
| COLOR | COLOR | Integer | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_BASE\_LAYER | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| ID | ID | Integer | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_BASEMAP\_REFRESH | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| DEPT\_ID | Department ID | SmallInteger | 2 |  |
| DEPT\_NAME | Department Name | String | 50 |  |
| CONT\_NAME | Contact Name | String | 50 |  |
| CONT\_PHONE | Contact Phone | String | 20 |  |
| CONT\_EMAIL | Contact Email | String | 40 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| GBME\_BRIDGE | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| SURFACEM | Surface Material | String | 16 | CodeSurfaceMaterial |
| DESCRIP | Description | String | 255 |  |
| BRIDGETYPE | Bridge Type | String | 16 | CodeBridgeType |
| VERTICAL | Vertical Structure Material | String | 16 | CodeVerticalStructureMaterial |
| DIRECTION | Directionality | String | 16 | CodeDirectionality |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| USERFLAG | User Flag | String | 254 |  |
| COMMENTS | Comments | String | 150 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| Z\_MIN | Z\_MIN | Double | 8 |  |
| Z\_MAX | Z\_MAX | Double | 8 |  |
| Z\_MEAN | Z\_MEAN | Double | 8 |  |
| SHAPE | Shape | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_CITY\_BOUNDARY | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| AREA | AREA | Double | 8 |  |
| PERIMETER | PERIMETER | Double | 8 |  |
| NAME | NAME | String | 50 |  |
| SRC\_DOC | SRC\_DOC | String | 30 |  |
| SRC\_SCALE | SRC\_SCALE | String | 5 |  |
| SRC\_AGENCY | SRC\_AGENCY | String | 6 |  |
| SRC\_COMMEN | SRC\_COMMEN | String | 50 |  |
| SRC\_DATE | SRC\_DATE | String | 10 |  |
| REV\_DATE | REV\_DATE | String | 10 |  |
| UNINCORPOR | UNINCORPOR | SmallInteger | 2 |  |
| ABBR | ABBR | String | 3 |  |
| HANSEN\_ARE | HANSEN\_ARE | String | 50 |  |
| GEOMETRY\_A | GEOMETRY\_A | Double | 8 |  |
| GEOMETRY\_L | GEOMETRY\_L | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_EMASS | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| ID | Id | Integer | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_GARAGE\_L1 | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| LAYER | LAYER | String | 254 |  |
| BUILDING | BUILDING | String | 50 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_GARAGE\_L2 | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| LAYER | LAYER | String | 254 |  |
| BUILDING | BUILDING | String | 50 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_GARAGE\_L3 | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| LAYER | LAYER | String | 254 |  |
| BUILDING | BUILDING | String | 50 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_GARAGE\_L4 | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| LAYER | LAYER | String | 254 |  |
| BUILDING | BUILDING | String | 50 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_GARAGE\_L5 | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| LAYER | LAYER | String | 254 |  |
| BUILDING | BUILDING | String | 50 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_GARAGE\_L6 | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| LAYER | LAYER | String | 254 |  |
| BUILDING | BUILDING | String | 50 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_GARAGE\_L7 | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| LAYER | LAYER | String | 254 |  |
| BUILDING | BUILDING | String | 50 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_GARAGE\_L8 | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| LAYER | LAYER | String | 254 |  |
| BUILDING | BUILDING | String | 50 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_GARAGE\_L9 | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| LAYER | LAYER | String | 254 |  |
| BUILDING | BUILDING | String | 50 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_LEADER\_LINE | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_LIGHTING\_PIER | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| NAME | Name | String | 50 |  |
| DESCRIP | Description | String | 255 |  |
| STATUS | Status | String | 20 | CodeStatus |
| USERFLAG | User Flag | String | 254 |  |
| SURFACEM | Surface Material | String | 16 |  |
| BRIDGETYPE | Bridge Type | String | 16 |  |
| VERTICAL | Vertical Structure Material | String | 16 | CodeVerticalStructureMaterial |
| DIRECTION | Directionality | String | 16 | CodeDirectionality |
| ALTERNATIV | Alternative | Integer | 4 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| CADDLAYERNAME | CADDLAYERNAME | String | 40 |  |
| CADDLAYERDESC | CADDLAYERDESC | String | 50 |  |
| CADDCOLOR | CADDCOLOR | Integer | 4 |  |
| DATEDATAACQUIRED | DATEDATAACQUIRED | Date | 8 |  |
| DATASOURCE | DATASOURCE | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | Shape | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_MARKING\_LINE | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| LAYER | LAYER | String | 254 |  |
| SHAPE\_LENG | SHAPE\_LENG | Double | 8 |  |
| FID\_ | FID\_ | Integer | 4 |  |
| ENTITY | ENTITY | String | 16 |  |
| COLOR | COLOR | Integer | 4 |  |
| LINETYPE | LINETYPE | String | 254 |  |
| ELEVATION | ELEVATION | Double | 8 |  |
| LINEWT | LINEWT | Integer | 4 |  |
| REFNAME | REFNAME | String | 254 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| NAME | Name | String | 40 |  |
| CATEGORY | Category | String | 20 |  |
| DESCRIPTION | Description | String | 50 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_MOVEMENT\_AREA\_LINE | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| DESCRIP | Description | String | 255 |  |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| COMMENTS | Comments | String | 150 |  |
| USERFLAG | User Flag | String | 254 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | Shape | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_PARKING\_AREA | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| AREA | AREA | String | 50 |  |
| GID | GID | Integer | 4 |  |
| NAME | NAME | String | 50 |  |
| PARCUSE | PARCUSE | String | 16 |  |
| DESCRIP | DESCRIP | String | 254 |  |
| TOTSPACES | TOTSPACES | Integer | 4 |  |
| NOHNDCPSP | NOHNDCPSP | Integer | 4 |  |
| OWNER | OWNER | String | 16 |  |
| SURFACET | SURFACET | String | 16 |  |
| STATUS | STATUS | String | 20 |  |
| ALTERNATIV | ALTERNATIV | Integer | 4 |  |
| USERFLAG | USERFLAG | String | 254 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| CADDLAYERN | CADDLAYERN | String | 40 |  |
| CADDLAYERD | CADDLAYERD | String | 50 |  |
| CADDCOLOR | CADDCOLOR | Integer | 4 |  |
| DATEDATAAC | DATEDATAAC | Date | 8 |  |
| DATASOURCE | DATASOURCE | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE\_LENG | SHAPE\_LENG | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_PASSENGER\_LOADING\_BRIDGE | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| DESCRIP | Description | String | 255 |  |
| LOADINGBT | Loading Bridge Type | String | 16 | CodeLoadingBridgeType |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| COMMENTS | Comments | String | 150 |  |
| USERFLAG | User Flag | String | 254 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | Shape | Geometry | 0 |  |
| GATE\_ID\_1 | GATE\_ID\_1 | String | 10 |  |
| GATE\_ID\_2 | GATE\_ID\_2 | String | 10 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_PUBLIC\_ROAD | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FULL\_NAME | FULL\_NAME | String | 69 |  |
| PREFIX | PREFIX | String | 6 |  |
| NAME | NAME | String | 50 |  |
| TYPE | TYPE | String | 4 |  |
| SUFFIX | SUFFIX | String | 6 |  |
| STNA\_ID | STNA\_ID | Double | 8 |  |
| LENGTH | LENGTH | Double | 8 |  |
| FR\_ADD\_L | FR\_ADD\_L | Double | 8 |  |
| TO\_ADD\_L | TO\_ADD\_L | Double | 8 |  |
| FR\_ADD\_R | FR\_ADD\_R | Double | 8 |  |
| TO\_ADD\_R | TO\_ADD\_R | Double | 8 |  |
| ADD\_100\_LO | ADD\_100\_LO | Double | 8 |  |
| ADD\_100\_HI | ADD\_100\_HI | Double | 8 |  |
| CITY\_L | CITY\_L | String | 10 |  |
| CITY\_R | CITY\_R | String | 10 |  |
| ZIP\_L | ZIP\_L | Double | 8 |  |
| ZIP\_R | ZIP\_R | Double | 8 |  |
| ERROR\_FLAG | ERROR\_FLAG | Double | 8 |  |
| TW\_FLAG | TW\_FLAG | Double | 8 |  |
| SRC\_DOC | SRC\_DOC | String | 30 |  |
| SRC\_DATE | SRC\_DATE | String | 10 |  |
| SRC\_SCALE | SRC\_SCALE | String | 5 |  |
| SRC\_AGENCY | SRC\_AGENCY | String | 6 |  |
| SRC\_COMMEN | SRC\_COMMEN | String | 50 |  |
| REV\_DATE | REV\_DATE | String | 10 |  |
| OFFSET | OFFSET | String | 1 |  |
| STCONO | STCONO | String | 10 |  |
| RD\_NO | RD\_NO | String | 5 |  |
| CNTY\_MAINT | CNTY\_MAINT | String | 1 |  |
| STNALIST\_S | STNALIST\_S | Double | 8 |  |
| ROUTE\_ID | ROUTE\_ID | String | 50 |  |
| LOW\_MEASUR | LOW\_MEASUR | Double | 8 |  |
| HI\_MEASURE | HI\_MEASURE | Double | 8 |  |
| LRS\_REVERS | LRS\_REVERS | Double | 8 |  |
| GEOMETRY\_L | GEOMETRY\_L | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_RAILWAY\_CENTERLINE | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| DESCRIP | Description | String | 255 |  |
| NUMTRACKS | Number Of Tracks | Integer | 4 |  |
| OWNER | Owner | String | 16 | CodeOwner |
| ISBRIDGE | Is Bridge | String | 1 | CodeBoolean |
| ISTUNNEL | Is Tunnel | String | 1 | CodeBoolean |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| COMMENTS | Comments | String | 150 |  |
| USERFLAG | User Flag | String | 254 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DIRECTION | Directionality | String | 16 | CodeDirectionality |
| SEGMENTT | Segment Type | String | 16 | CodeSegmentType |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_RUNWAY\_ELEMENT | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | GID | Integer | 4 |  |
| NAME | NAME | String | 50 |  |
| DESCRIP | DESCRIP | String | 254 |  |
| RWYDESG | RWYDESG | String | 7 |  |
| WIDTH | WIDTH | Double | 8 |  |
| LENGTH | LENGTH | Double | 8 |  |
| SURFACET | SURFACET | String | 16 |  |
| SURFACEM | SURFACEM | String | 16 |  |
| PAVEMENTCL | PAVEMENTCL | String | 10 |  |
| SURFACEC | SURFACEC | String | 16 |  |
| STATUS | STATUS | String | 20 |  |
| ALTERNATIV | ALTERNATIV | Integer | 4 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| USERFLAG | USERFLAG | String | 254 |  |
| CADDLAYERN | CADDLAYERN | String | 40 |  |
| CADDLAYERD | CADDLAYERD | String | 50 |  |
| CADDCOLOR | CADDCOLOR | Integer | 4 |  |
| DATEDATAAC | DATEDATAAC | Date | 8 |  |
| DATASOURCE | DATASOURCE | String | 50 |  |
| SHAPE\_LENG | Shape\_Leng | Double | 8 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_SFO\_ROADWAY | | | | |
| OBJECTID | FID | OID | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_SFO\_ROADWAY\_MARKING\_LINE | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FID\_ | FID\_ | Integer | 4 |  |
| ENTITY | ENTITY | String | 16 |  |
| HANDLE | HANDLE | String | 16 |  |
| LAYER | LAYER | String | 254 |  |
| LYRFRZN | LYRFRZN | Integer | 4 |  |
| LYRLOCK | LYRLOCK | Integer | 4 |  |
| LYRON | LYRON | Integer | 4 |  |
| LYRVPFRZN | LYRVPFRZN | Integer | 4 |  |
| LYRHANDLE | LYRHANDLE | String | 16 |  |
| COLOR | COLOR | Integer | 4 |  |
| ENTCOLOR | ENTCOLOR | Integer | 4 |  |
| LYRCOLOR | LYRCOLOR | Integer | 4 |  |
| BLKCOLOR | BLKCOLOR | Integer | 4 |  |
| LINETYPE | LINETYPE | String | 254 |  |
| ENTLINETYP | ENTLINETYP | String | 254 |  |
| LYRLNTYPE | LYRLNTYPE | String | 254 |  |
| BLKLINETYP | BLKLINETYP | String | 254 |  |
| ELEVATION | ELEVATION | Double | 8 |  |
| THICKNESS | THICKNESS | Double | 8 |  |
| LINEWT | LINEWT | Integer | 4 |  |
| ENTLINEWT | ENTLINEWT | Integer | 4 |  |
| LYRLINEWT | LYRLINEWT | Integer | 4 |  |
| BLKLINEWT | BLKLINEWT | Integer | 4 |  |
| REFNAME | REFNAME | String | 254 |  |
| LTSCALE | LTSCALE | Double | 8 |  |
| EXTX | EXTX | Double | 8 |  |
| EXTY | EXTY | Double | 8 |  |
| EXTZ | EXTZ | Double | 8 |  |
| DOCNAME | DOCNAME | String | 254 |  |
| DOCPATH | DOCPATH | String | 254 |  |
| DOCTYPE | DOCTYPE | String | 32 |  |
| DOCVER | DOCVER | String | 16 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_SHORELINE\_BAY | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| DESCRIP | Description | String | 255 |  |
| SHORETYPE | Shoreline Type | String | 16 |  |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| COMMENTS | Comments | String | 150 |  |
| USERFLAG | User Flag | String | 254 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | Shape | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_SHORELINE\_SFO | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| DESCRIP | Description | String | 255 |  |
| SHORETYPE | Shoreline Type | String | 16 |  |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| COMMENTS | Comments | String | 150 |  |
| USERFLAG | User Flag | String | 254 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | Shape | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_SHOULDER\_ELEMENT | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| ENTITY | ENTITY | String | 16 |  |
| LAYER | LAYER | String | 255 |  |
| COLOR | COLOR | SmallInteger | 2 |  |
| LINETYPE | LINETYPE | String | 255 |  |
| ELEVATION | ELEVATION | Double | 8 |  |
| LINEWT | LINEWT | SmallInteger | 2 |  |
| REFNAME | REFNAME | String | 255 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| CONTRACT\_NUMBER | CONTRACT\_NUMBER | String | 30 |  |
| CONTRACT\_YEAR | CONTRACT\_YEAR | String | 20 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 30 |  |
| DATE\_ENTERED | DATE\_ENTERED | String | 20 |  |
| DRAWING\_ID | DRAWING\_ID | String | 255 |  |
| LAYER\_DESC | LAYER\_DESC | String | 50 |  |
| PROJECT\_MANAGER | PROJECT\_MANAGER | String | 30 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_STRUCTURES\_PUBLIC | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| LAYER\_DESC | LAYER\_DESC | String | 254 |  |
| SHAPE | Shape | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_STRUCTURES\_ROOF | | | | |
| OBJECTID | GID | OID | 4 |  |
| GEOM\_AREA | GEOM\_AREA | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| DESCRIP | DESCRIP | String | 255 |  |
| BUILDINGNO | BUILDINGNO | String | 16 |  |
| STATUS | STATUS | String | 20 |  |
| USERFLAG | USERFLAG | String | 254 |  |
| CAD\_LAYNAME | CAD\_LAYNAME | String | 40 |  |
| CAD\_LAYDESC | CAD\_LAYDESC | String | 50 |  |
| DATE\_ACQUIRED | DATE\_ACQUIRED | Date | 8 |  |
| DATA\_SOURCE | DATA\_SOURCE | String | 25 |  |
| NAME | NAME | String | 50 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| ALTERNATIV | ALTERNATIV | Double | 8 |  |
| CAD\_LAYCOLOR | CAD\_LAYCOLOR | Double | 8 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| GEOMETRY\_Area | GEOMETRY\_Area | Double | 8 |  |
| GBME\_TANK\_SITE | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| TANKTYPE | Tank Type | String | 40 |  |
| DESCRIP | Description | String | 255 |  |
| TOPELEV | Top Elevation | Double | 8 |  |
| LIGHTCODE | Light Code | String | 1 | CodeBoolean |
| VERTICAL | Vertical Structure Material | String | 16 | CodeVerticalStructureMaterial |
| LIGHTING | Lighting Type | String | 16 | CodeLightingConfigurationType |
| MARKINGF | Marking Feature Type | String | 17 | CodeMarkingFeatureType |
| COLOR | Color | String | 16 | CodeColor |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| COMMENTS | Comments | String | 150 |  |
| USERFLAG | User Flag | String | 254 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | Shape | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_TAXIWAY\_ELEMENT | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| DESCRIP | Description | String | 255 |  |
| TAXIWAYID | Taxiway ID | String | 50 |  |
| TAXIWAYT | Taxiway Type | String | 18 | CodeTaxiwayType |
| SURFACEM | Surface Material | String | 16 | CodeSurfaceMaterial |
| PAVEMENTCL | Pavement Classification Number | String | 10 |  |
| SURFACEC | Surface Condition | String | 16 | CodeSurfaceCondition |
| DIRECTION | Directionality | String | 16 | CodeDirectionality |
| SEQUENCE | Sequence | String | 5 |  |
| SURFACET | Surface Type | String | 16 | CodeSurfaceType |
| DESIGNGR | Design Group | String | 16 | CodeDesignGroup |
| LENGTH | Length | Double | 8 |  |
| WIDTH | Width | Double | 8 |  |
| MAXSPEED | Maximum Speed | Integer | 4 |  |
| WINGSPAN | Wingspan | Double | 8 |  |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| USERFLAG | User Flag | String | 254 |  |
| COMMENTS | Comments | String | 150 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBME\_TAXIWAY\_HOLDING\_POSITION | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | Global Unique Id | Integer | 4 |  |
| NAME | Name | String | 50 |  |
| DESCRIP | Description | String | 255 |  |
| RWYDESG | Runway Designator | String | 7 |  |
| TAXIDESGN | Taxiway Designator | String | 4 |  |
| LOWVISCAT | Low Visibility Category | String | 16 |  |
| STATUS | Status | String | 20 | CodeStatus |
| ALTERNATIV | Alternative | Integer | 4 |  |
| COMMENTS | Comments | String | 150 |  |
| USERFLAG | User Flag | String | 254 |  |
| CADDLAYERNAME | CADD Layer Name | String | 40 |  |
| CADDLAYERDESC | CADD Layer Description | String | 50 |  |
| CADDCOLOR | CADD Layer Color | Integer | 4 |  |
| DATEDATAACQUIRED | Date Data Acquired | Date | 8 |  |
| DATASOURCE | Data Source | String | 50 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| LAYER | LAYER | String | 50 |  |
| LYRCOLOR | LYRCOLOR | SmallInteger | 2 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_VSR\_AARF\_RESTRICTED | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| GID | GID | Integer | 4 |  |
| NAME | NAME | String | 50 |  |
| DESCRIP | DESCRIP | String | 254 |  |
| COLOR | COLOR | String | 16 |  |
| STATUS | STATUS | String | 20 |  |
| ALTERNATIV | ALTERNATIV | Integer | 4 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| USERFLAG | USERFLAG | String | 254 |  |
| CADDLAYERN | CADDLAYERN | String | 40 |  |
| CADDLAYERD | CADDLAYERD | String | 50 |  |
| CADDCOLOR | CADDCOLOR | Integer | 4 |  |
| DATEDATAAC | DATEDATAAC | Date | 8 |  |
| DATASOURCE | DATASOURCE | String | 50 |  |
| SHAPE\_LENG | Shape\_Leng | Double | 8 |  |
| QA\_ID | QA\_ID | String | 50 |  |
| SHAPE | Shape | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBME\_VSR\_VEHICLE\_SERVICE\_ROAD | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | GID | Double | 8 |  |
| GEOM\_LENGT | GEOM\_LENGT | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 20 |  |
| LAYER\_DESC | LAYER\_DESC | String | 50 |  |
| CONTRACT\_N | CONTRACT\_N | String | 30 |  |
| CONTRACT\_Y | CONTRACT\_Y | String | 20 |  |
| DATA\_SOURC | DATA\_SOURC | String | 30 |  |
| PROJECT\_MA | PROJECT\_MA | String | 30 |  |
| DATE\_ENTER | DATE\_ENTER | Date | 8 |  |
| DRAWING\_ID | DRAWING\_ID | String | 150 |  |
| PARENT\_GID | PARENT\_GID | Double | 8 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_II\_AIRTRAIN\_SPACES | | | | |
| OBJECTID\_1 | FID | OID | 4 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| ENTITY | ENTITY | String | 16 |  |
| LAYER | Layer | String | 254 |  |
| COLOR | Color | Integer | 4 |  |
| LINETYPE | Linetype | String | 254 |  |
| ELEVATION | Elevation | Double | 8 |  |
| LINEWT | LineWt | Integer | 4 |  |
| REFNAME | RefName | String | 254 |  |
| NAME | Name | String | 200 |  |
| SHAPE\_LENG | Shape\_Leng | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBMI\_II\_CENTRAL\_GARAGE\_SPACES | | | | |
| OBJECTID\_1 | FID | OID | 4 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| ENTITY | ENTITY | String | 16 |  |
| LAYER | Layer | String | 254 |  |
| COLOR | Color | Integer | 4 |  |
| LINETYPE | Linetype | String | 254 |  |
| ELEVATION | Elevation | Double | 8 |  |
| LINEWT | LineWt | Integer | 4 |  |
| REFNAME | RefName | String | 254 |  |
| NAME | Name | String | 50 |  |
| LOCATION | Location | String | 50 |  |
| LEVEL\_ | Level | String | 10 |  |
| SHAPE\_LENG | Shape\_Leng | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBMI\_II\_TERMINAL\_ITB\_L3\_SPACES | | | | |
| OBJECTID\_1 | FID | OID | 4 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| ENTITY | ENTITY | String | 16 |  |
| LAYER | Layer | String | 254 |  |
| COLOR | Color | Integer | 4 |  |
| LINETYPE | Linetype | String | 254 |  |
| ELEVATION | Elevation | Double | 8 |  |
| LINEWT | LineWt | Integer | 4 |  |
| REFNAME | RefName | String | 254 |  |
| NAME | Name | String | 250 |  |
| SECURITY | Security | String | 50 |  |
| SHAPE\_LENG | Shape\_Leng | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBMI\_II\_TERMINAL\_L1\_SPACES | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| OID\_ | OID\_ | Integer | 4 |  |
| NAME | NAME | String | 254 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBMI\_II\_TERMINAL\_L2\_SPACES | | | | |
| OBJECTID\_1 | FID | OID | 4 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| ENTITY | ENTITY | String | 16 |  |
| LAYER | Layer | String | 254 |  |
| COLOR | Color | Integer | 4 |  |
| LINETYPE | Linetype | String | 254 |  |
| ELEVATION | Elevation | Double | 8 |  |
| LINEWT | LineWt | Integer | 4 |  |
| REFNAME | RefName | String | 254 |  |
| NAME | Name | String | 200 |  |
| SECURITY | Security | String | 50 |  |
| SHAPE\_LENG | Shape\_Leng | Double | 8 |  |
| APPRX\_AREA | APPRX\_AREA | Double | 8 |  |
| TYPE | TYPE | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBMI\_II\_TERMINAL\_L3\_SPACES | | | | |
| OBJECTID\_1 | FID | OID | 4 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| ENTITY | ENTITY | String | 16 |  |
| LAYER | Layer | String | 254 |  |
| COLOR | Color | Integer | 4 |  |
| LINETYPE | Linetype | String | 254 |  |
| ELEVATION | Elevation | Double | 8 |  |
| LINEWT | LineWt | Integer | 4 |  |
| REFNAME | RefName | String | 254 |  |
| NAME | Name | String | 200 |  |
| SECURITY | Security | String | 50 |  |
| SHAPE\_LENG | Shape\_Leng | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBMI\_L1\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| ARCGIS\_HS\_BLDG\_LV1\_V2\_ENTITY | ARCGIS.HS\_Bldg\_Lv1\_v2.ENTITY | String | 16 |  |
| LAYER | LAYER | String | 255 |  |
| COLOR | COLOR | SmallInteger | 2 |  |
| LINETYPE | LINETYPE | String | 255 |  |
| ELEVATION | ELEVATION | Double | 8 |  |
| LINEWT | LINEWT | SmallInteger | 2 |  |
| REFNAME | REFNAME | String | 255 |  |
| ARCGIS\_HS\_BLDG\_LV1\_ENTITY | ARCGIS\_HS\_BLDG\_LV1\_ENTITY | String | 16 |  |
| LEVEL\_ | Floor Level | String | 50 |  |
| ENTITY\_1 | ENTITY\_1 | String | 16 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_L2\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| LAYER | LAYER | String | 255 |  |
| COLOR | COLOR | SmallInteger | 2 |  |
| REFNAME | REFNAME | String | 255 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_L3\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| LAYER | LAYER | String | 255 |  |
| REFNAME | REFNAME | String | 255 |  |
| FLOOR\_ | FLOOR\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_PME\_ELECTRIC\_WALWAY | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| PEOPLE\_MOVERS\_ID | People Movers ID | String | 50 |  |
| FLOOR\_LEVEL | Floor Level | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| GBMI\_PME\_ELEVATOR | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| ELEVATOR\_ID | Elevator ID | String | 50 |  |
| FLOOR\_LEVEL | Floor Level | String | 50 |  |
| NOTES | NOTES | String | 100 |  |
| CONFIRMATION | Confirmation | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| GBMI\_PME\_ESCALATOR | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| ESCALATORS\_ID | Escalators ID | String | 50 |  |
| FLOOR\_LEVEL | Floor Level | String | 50 |  |
| NOTES | NOTES | String | 200 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| GBMI\_TERMINAL\_BASEMENT\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| REFNAME | REFNAME | String | 255 |  |
| BUILDING | BUILDING | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_TERMINAL\_ITBMEZZ\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| BUILDING | BUILDING | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_TERMINAL\_L1\_FP | | | | |
| OBJECTID\_12 | OBJECTID\_12 | OID | 4 |  |
| FID\_ | FID\_ | Integer | 4 |  |
| OBJECTID\_1 | OBJECTID\_1 | Integer | 4 |  |
| BUILDING | BUILDING | String | 50 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| SHAPE\_LENG | SHAPE\_LENG | Double | 8 |  |
| ROTATE | ROTATE | Double | 8 |  |
| SHAPE\_LE\_1 | SHAPE\_LE\_1 | Double | 8 |  |
| SHAPE\_LE\_2 | SHAPE\_LE\_2 | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| GBMI\_TERMINAL\_L1\_FP | | | | |
| OBJECTID | OBJECTID | Integer | 4 |  |
| BUILDING | BUILDING | String | 50 |  |
| SHAPE\_LENG | SHAPE\_LENG | Double | 8 |  |
| ROTATE | ROTATE | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_TERMINAL\_L3\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| BUILDING | BUILDING | String | 50 |  |
| ROTATE | ROTATE | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_TERMINAL\_L3M\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| BUILDING | BUILDING | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_TERMINAL\_L4\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| REFNAME | REFNAME | String | 255 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_TERMINAL\_L5\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| BUILDING | BUILDING | String | 100 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_TERMINAL\_L6\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FACP | FACP | String | 6 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| GBMI\_TERMINAL\_SPACES | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| SPACE\_KEY | SPACE\_KEY | SmallInteger | 2 |  |
| ROOM\_ID\_ | ROOM\_ID\_ | String | 50 |  |
| SPACE\_TYPE\_ | SPACE\_TYPE\_ | String | 100 |  |
| SPACE\_SUBTYPE\_ | SPACE\_SUBTYPE\_ | String | 100 |  |
| SPACE\_TENANT\_ | SPACE\_TENANT\_ | String | 100 |  |
| LEASE\_SQFT\_ | LEASE\_SQFT\_ | Integer | 4 |  |
| FLOOR\_LEVEL\_ | FLOOR\_LEVEL\_ | String | 50 |  |
| TERMINAL\_BUILDING | TERMINAL\_BUILDING | String | 50 |  |
| FLOOR\_TYPE\_ | FLOOR\_TYPE\_ | String | 50 |  |
| SECURITY\_ | SECURITY\_ | String | 50 |  |
| DATE\_ | DATE\_ | Date | 8 |  |
| LINK | LINK | String | 500 |  |
| PHOTO | PHOTO | String | 500 |  |
| LAYER | LAYER | String | 255 |  |
| DOCPATH | DOCPATH | String | 1025 |  |
| SECURITY | SECURITY | String | 10 |  |
| ACCESS\_ | ACCESS\_ | String | 20 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| CALC\_AREA | CALC\_AREA | Double | 8 |  |
| MAP\_CLASS | MAP\_CLASS | String | 50 |  |
| CADTYPE | CADTYPE | String | 50 |  |
| TXTVALUE | TXTVALUE | String | 50 |  |
| MAP\_LABEL | MAP\_LABEL | String | 250 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBMI\_TERMINAL\_SPACES\_15 | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| SPACE\_KEY | SPACE\_KEY | SmallInteger | 2 |  |
| ROOM\_ID\_ | ROOM\_ID\_ | String | 50 |  |
| SPACE\_TYPE\_ | SPACE\_TYPE\_ | String | 100 |  |
| SPACE\_SUBTYPE\_ | SPACE\_SUBTYPE\_ | String | 100 |  |
| SPACE\_TENANT\_ | SPACE\_TENANT\_ | String | 100 |  |
| LEASE\_SQFT\_ | LEASE\_SQFT\_ | Integer | 4 |  |
| FLOOR\_LEVEL\_ | FLOOR\_LEVEL\_ | String | 50 |  |
| TERMINAL\_BUILDING | TERMINAL\_BUILDING | String | 50 |  |
| FLOOR\_TYPE\_ | FLOOR\_TYPE\_ | String | 50 |  |
| SECURITY\_ | SECURITY\_ | String | 50 |  |
| DATE\_ | DATE\_ | Date | 8 |  |
| LINK | LINK | String | 500 |  |
| PHOTO | PHOTO | String | 500 |  |
| LAYER | LAYER | String | 255 |  |
| DOCPATH | DOCPATH | String | 1025 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| GBMI\_TUNNEL\_FP | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| REFNAME | REFNAME | String | 255 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| LAND\_IRRIGATION\_LINES | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| ID | Id | Integer | 4 |  |
| NAME | NAME | String | 50 |  |
| COMMENTS | COMMENTS | String | 500 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| LAND\_IRRIGATION\_VALVE | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| TYPE | Type | SmallInteger | 2 |  |
| NOTES | Notes | String | 200 |  |
| DATE\_ | Date | Date | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| NOISE\_SMC\_ASSESSOR | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GEOM\_AREA | GEOM\_AREA | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| APN | APN | String | 9 |  |
| TRA | TRA | String | 6 |  |
| OWNER1 | OWNER1 | String | 40 |  |
| OWNER2 | OWNER2 | String | 40 |  |
| OWNER3 | OWNER3 | String | 40 |  |
| MAIL\_ADDRESS1 | MAIL\_ADDRESS1 | String | 60 |  |
| MAIL\_ADDRESS2 | MAIL\_ADDRESS2 | String | 60 |  |
| MAIL\_ADDRESS3 | MAIL\_ADDRESS3 | String | 60 |  |
| MAIL\_CITY | MAIL\_CITY | String | 20 |  |
| MAIL\_STATE | MAIL\_STATE | String | 2 |  |
| MAIL\_ZIP | MAIL\_ZIP | String | 9 |  |
| MAIL\_COUNTRY | MAIL\_COUNTRY | String | 4 |  |
| SITUS\_NO1 | SITUS\_NO1 | String | 8 |  |
| SITUS\_NO2 | SITUS\_NO2 | String | 8 |  |
| SITUS\_FRACTION | SITUS\_FRACTION | String | 3 |  |
| SITUS\_DIRECTION | SITUS\_DIRECTION | String | 3 |  |
| SITUS\_STREET | SITUS\_STREET | String | 32 |  |
| SITUS\_STREET\_TY | SITUS\_STREET\_TY | String | 4 |  |
| SITUS\_STREET\_BOX | SITUS\_STREET\_BOX | String | 8 |  |
| SITUS\_CITY | SITUS\_CITY | String | 20 |  |
| PUC\_CODE | PUC\_CODE | String | 2 |  |
| DATE\_RECORD | DATE\_RECORD | Date | 8 |  |
| DOCUMENT\_NO | DOCUMENT\_NO | String | 11 |  |
| DATE\_SALE | DATE\_SALE | Date | 8 |  |
| AMOUNT\_SALE | AMOUNT\_SALE | Double | 8 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| PLAN\_COMPOSITE | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| LAYER | LAYER | String | 50 |  |
| LAYER\_DESC | LAYER\_DESC | String | 50 |  |
| ELEVATION | ELEVATION | Integer | 4 |  |
| DOC\_SOURCE | DOC\_SOURCE | String | 30 |  |
| DOC\_DATE | DOC\_DATE | Date | 8 |  |
| CREATED\_USER | CREATED\_USER | String | 255 |  |
| CREATED\_DATE | CREATED\_DATE | Date | 8 |  |
| LAST\_EDITED\_USER | LAST\_EDITED\_USER | String | 255 |  |
| LAST\_EDITED\_DATE | LAST\_EDITED\_DATE | Date | 8 |  |
| CADLAYN18B | CADLAYN18B | String | 20 |  |
| DATAORIGIN | DATAORIGIN | String | 50 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| PLAN\_OEAAA\_OFF | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| LAYER | LAYER | String | 30 |  |
| LAYER\_DESC | LAYER\_DESC | String | 50 |  |
| STUDY\_ASN | STUDY\_ASN | String | 20 |  |
| STATUS | STATUS | String | 15 |  |
| DETERMINATION | DETERMINATION | String | 15 |  |
| LATITUDE | LATITUDE | String | 20 |  |
| LONGITUDE | LONGITUDE | String | 20 |  |
| STRUCTURE\_NAME | STRUCTURE\_NAME | String | 50 |  |
| CITY | CITY | String | 30 |  |
| AGL\_HT\_DET | AGL\_HT\_DET | SmallInteger | 2 |  |
| AMSL\_HT\_DET | AMSL\_HT\_DET | SmallInteger | 2 |  |
| DOC\_SOURCE | DOC\_SOURCE | String | 30 |  |
| DOC\_DATE | DOC\_DATE | Date | 8 |  |
| CREATED\_USER | CREATED\_USER | String | 255 |  |
| CREATED\_DATE | CREATED\_DATE | Date | 8 |  |
| LAST\_EDITED\_USER | LAST\_EDITED\_USER | String | 255 |  |
| LAST\_EDITED\_DATE | LAST\_EDITED\_DATE | Date | 8 |  |
| CADLAYN18B | CADLAYN18B | String | 20 |  |
| DATAORIGIN | DATAORIGIN | String | 40 |  |
| STRUCTURE\_TYPE1 | STRUCTURE\_TYPE | String | 30 | PLAN\_OEAAA\_OFF\_STRUCTYPE |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| PLAN\_OEAAA\_ON | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| LAYER | LAYER | String | 30 |  |
| LAYER\_DESC | LAYER\_DESC | String | 50 |  |
| STUDY\_ASN | STUDY\_ASN | String | 20 |  |
| STATUS | STATUS | String | 15 |  |
| LATITUDE | LATITUDE | String | 20 |  |
| LONGITUDE | LONGITUDE | String | 20 |  |
| AGL\_HT | AGL\_HT | SmallInteger | 2 |  |
| SITE\_ELEV | SITE\_ELEV | SmallInteger | 2 |  |
| DOC\_SOURCE | DOC\_SOURCE | String | 30 |  |
| DOC\_DATE | DOC\_DATE | Date | 8 |  |
| CREATED\_USER | CREATED\_USER | String | 255 |  |
| CREATED\_DATE | CREATED\_DATE | Date | 8 |  |
| LAST\_EDITED\_USER | LAST\_EDITED\_USER | String | 255 |  |
| LAST\_EDITED\_DATE | LAST\_EDITED\_DATE | Date | 8 |  |
| STRUCTURE\_TYPE1 | STRUCTURE\_TYPE | String | 30 | PLAN\_OEAAA\_ON\_STRUCTYPE |
| CADLAYN18B | CADLAYN18B | String | 20 |  |
| DATAORIGIN | DATAORIGIN | String | 40 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| PLAN\_OEI | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GID | GID | Integer | 4 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| LAYER | LAYER | String | 50 |  |
| LAYER\_DESC | LAYER\_DESC | String | 50 |  |
| ELEVATION | ELEVATION | Integer | 4 |  |
| RUNWAY | RUNWAY | String | 10 |  |
| DOC\_SOURCE | DOC\_SOURCE | String | 30 |  |
| DOC\_DATE | DOC\_DATE | Date | 8 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| CREATED\_USER | CREATED\_USER | String | 255 |  |
| CREATED\_DATE | CREATED\_DATE | Date | 8 |  |
| LAST\_EDITED\_USER | LAST\_EDITED\_USER | String | 255 |  |
| LAST\_EDITED\_DATE | LAST\_EDITED\_DATE | Date | 8 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| PLAN\_PART77 | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| LAYER | LAYER | String | 50 |  |
| LAYER\_DESC | LAYER\_DESC | String | 50 |  |
| ELEVATION | ELEVATION | Integer | 4 |  |
| DOC\_SOURCE | DOC\_SOURCE | String | 30 |  |
| DOC\_DATE | DOC\_DATE | Date | 8 |  |
| CREATED\_USER | CREATED\_USER | String | 255 |  |
| CREATED\_DATE | CREATED\_DATE | Date | 8 |  |
| LAST\_EDITED\_USER | LAST\_EDITED\_USER | String | 255 |  |
| LAST\_EDITED\_DATE | LAST\_EDITED\_DATE | Date | 8 |  |
| CADLAYN18B | CADLAYN18B | String | 20 |  |
| DATAORIGIN | DATAORIGIN | String | 40 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| PLAN\_TERPS | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GEOM\_LENGTH | GEOM\_LENGTH | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| LAYER | LAYER | String | 50 |  |
| LAYER\_DESC | LAYER\_DESC | String | 50 |  |
| ELEVATION | ELEVATION | Integer | 4 |  |
| RUNWAY | RUNWAY | String | 5 |  |
| PROC\_TYPE | PROC\_TYPE | String | 30 |  |
| DOC\_SOURCE | DOC\_SOURCE | String | 30 |  |
| DOC\_DATE | DOC\_DATE | Date | 8 |  |
| CREATED\_USER | CREATED\_USER | String | 255 |  |
| CREATED\_DATE | CREATED\_DATE | Date | 8 |  |
| LAST\_EDITED\_USER | LAST\_EDITED\_USER | String | 255 |  |
| LAST\_EDITED\_DATE | LAST\_EDITED\_DATE | Date | 8 |  |
| CADLAYN18B | CADLAYN18B | String | 20 |  |
| DATAORIGIN | DATAORIGIN | String | 40 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| PSIM\_ACCESS\_CONTROL | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| NAME | NAME | String | 255 |  |
| AREA | AREA | String | 50 |  |
| TYPE | TYPE | String | 50 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| PSIM\_ACCESS\_CONTROL\_DETAIL | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| LAYER | LAYER | String | 21 |  |
| ELEVATION | ELEVATION | Double | 8 |  |
| DEVICE\_TYP | DEVICE\_TYP | String | 14 |  |
| DEV\_ID | DEV\_ID | Integer | 4 |  |
| NAME | NAME | String | 108 |  |
| CONNECTION | CONNECTION | String | 41 |  |
| MODEL\_NAME | MODEL\_NAME | String | 16 |  |
| SEVERITY | SEVERITY | String | 8 |  |
| INDOOR | INDOOR | SmallInteger | 2 |  |
| BUILDING | BUILDING | String | 21 |  |
| FLOOR | FLOOR | SmallInteger | 2 |  |
| HEIGHT | HEIGHT | Double | 8 |  |
| HEADING | HEADING | Double | 8 |  |
| INCLINATIO | INCLINATIO | Double | 8 |  |
| LENS\_NAME | LENS\_NAME | String | 10 |  |
| PTZ | PTZ | SmallInteger | 2 |  |
| VMD | VMD | SmallInteger | 2 |  |
| DOME | DOME | SmallInteger | 2 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| TYPE | TYPE | String | 50 |  |
| AREA | AREA | String | 50 |  |
| LABEL | LABEL | String | 500 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SECURITY\_ACCESS\_DEVICES | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| LAYER | LAYER | String | 21 |  |
| ELEVATION | ELEVATION | Double | 8 |  |
| DEVICE\_TYP | DEVICE\_TYP | String | 14 |  |
| DEV\_ID | DEV\_ID | Integer | 4 |  |
| NAME | NAME | String | 108 |  |
| CONNECTION | CONNECTION | String | 41 |  |
| MODEL\_NAME | MODEL\_NAME | String | 16 |  |
| SEVERITY | SEVERITY | String | 8 |  |
| INDOOR | INDOOR | SmallInteger | 2 |  |
| BUILDING | BUILDING | String | 21 |  |
| FLOOR | FLOOR | SmallInteger | 2 |  |
| HEIGHT | HEIGHT | Double | 8 |  |
| HEADING | HEADING | Double | 8 |  |
| INCLINATIO | INCLINATIO | Double | 8 |  |
| LENS\_NAME | LENS\_NAME | String | 10 |  |
| PTZ | PTZ | SmallInteger | 2 |  |
| VMD | VMD | SmallInteger | 2 |  |
| DOME | DOME | SmallInteger | 2 |  |
| LEVEL\_ | LEVEL\_ | String | 50 |  |
| TYPE | TYPE | String | 50 |  |
| AREA | AREA | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SFO\_B | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| TYPE | TYPE | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SFO\_LEVEL2\_SPACE\_DEMO | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| SPACE\_KEY | SPACE\_KEY | SmallInteger | 2 |  |
| ROOM\_ID\_ | ROOM\_ID\_ | String | 50 |  |
| SPACE\_TYPE\_ | SPACE\_TYPE\_ | String | 100 |  |
| SPACE\_SUBTYPE\_ | SPACE\_SUBTYPE\_ | String | 100 | SFO\_LEVEL2\_SPACE\_DEMO |
| SPACE\_TENANT\_ | SPACE\_TENANT\_ | String | 100 |  |
| LEASE\_SQFT\_ | LEASE\_SQFT\_ | Integer | 4 |  |
| FLOOR\_LEVEL\_ | FLOOR\_LEVEL\_ | String | 50 | FLOOR\_LEVEL |
| TERMINAL\_BUILDING | TERMINAL\_BUILDING | String | 50 |  |
| FLOOR\_TYPE\_ | FLOOR\_TYPE\_ | String | 50 | FLOOR\_TYPE |
| SECURITY\_ | SECURITY\_ | String | 50 |  |
| DATE\_ | DATE\_ | Date | 8 |  |
| LINK | LINK | String | 500 |  |
| PHOTO | PHOTO | String | 500 |  |
| LAYER | LAYER | String | 255 |  |
| DOCPATH | DOCPATH | String | 1025 |  |
| SECURITY | SECURITY | String | 10 |  |
| ACCESS\_ | ACCESS\_ | String | 20 |  |
| CALC\_AREA | CALC\_AREA | Double | 8 |  |
| MAP\_CLASS | MAP\_CLASS | String | 50 |  |
| CADTYPE | CADTYPE | String | 50 |  |
| TXTVALUE | TXTVALUE | String | 50 |  |
| MAP\_LABEL | MAP\_LABEL | String | 250 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| SP\_SMC\_ASSESSOR | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| GEOM\_AREA | GEOM\_AREA | Double | 8 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| TAG\_X | TAG\_X | Double | 8 |  |
| TAG\_Y | TAG\_Y | Double | 8 |  |
| TAG\_VALUE | TAG\_VALUE | String | 40 |  |
| TAG\_SIZE | TAG\_SIZE | Double | 8 |  |
| TAG\_ANGLE | TAG\_ANGLE | Double | 8 |  |
| TAG\_JUST | TAG\_JUST | String | 2 |  |
| APN | APN | String | 9 |  |
| TRA | TRA | String | 6 |  |
| OWNER1 | OWNER1 | String | 40 |  |
| OWNER2 | OWNER2 | String | 40 |  |
| OWNER3 | OWNER3 | String | 40 |  |
| MAIL\_ADDRESS1 | MAIL\_ADDRESS1 | String | 60 |  |
| MAIL\_ADDRESS2 | MAIL\_ADDRESS2 | String | 60 |  |
| MAIL\_ADDRESS3 | MAIL\_ADDRESS3 | String | 60 |  |
| MAIL\_CITY | MAIL\_CITY | String | 20 |  |
| MAIL\_STATE | MAIL\_STATE | String | 2 |  |
| MAIL\_ZIP | MAIL\_ZIP | String | 9 |  |
| MAIL\_COUNTRY | MAIL\_COUNTRY | String | 4 |  |
| SITUS\_NO1 | SITUS\_NO1 | String | 8 |  |
| SITUS\_NO2 | SITUS\_NO2 | String | 8 |  |
| SITUS\_FRACTION | SITUS\_FRACTION | String | 3 |  |
| SITUS\_DIRECTION | SITUS\_DIRECTION | String | 3 |  |
| SITUS\_STREET | SITUS\_STREET | String | 32 |  |
| SITUS\_STREET\_TY | SITUS\_STREET\_TY | String | 4 |  |
| SITUS\_STREET\_BOX | SITUS\_STREET\_BOX | String | 8 |  |
| SITUS\_CITY | SITUS\_CITY | String | 20 |  |
| PUC\_CODE | PUC\_CODE | String | 2 |  |
| DATE\_RECORD | DATE\_RECORD | Date | 8 |  |
| DOCUMENT\_NO | DOCUMENT\_NO | String | 11 |  |
| DATE\_SALE | DATE\_SALE | Date | 8 |  |
| AMOUNT\_SALE | AMOUNT\_SALE | Double | 8 |  |
| PARENT\_GID | PARENT\_GID | Integer | 4 |  |
| DATE\_STAMP | DATE\_STAMP | Date | 8 |  |
| GEOMETRY | GEOMETRY | Geometry | 0 |  |
| GEOMETRY\_Length | GEOMETRY\_Length | Double | 8 |  |
| GEOMETRY\_Area | GEOMETRY\_Area | Double | 8 |  |
| SSR | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| ROOM\_ID | Room Number | String | 50 |  |
| CONDUCTED\_ON | Conducted On | Date | 8 |  |
| PREPARED\_BY | Prepared By | String | 50 |  |
| ACS\_DOOR\_SRVY | ACS Door Survey Completed | String | 10 |  |
| EP\_PRESENT | E-Power Present | String | 10 |  |
| EP\_CIRCUIT\_NUM | E-Power Circuit Numbers | String | 100 |  |
| EP\_SPACE\_AVAIL | E-Power Available Space | String | 10 |  |
| LSLAN\_PRESENT | Legacy S-LAN Present | String | 10 |  |
| LSLAN\_SWITCH\_NAME | Legacy S-LAN Switch Name | String | 100 |  |
| LSLAN\_SWITCH\_MANUFAC | Legacy S-LAN Switch Manufacturer | String | 100 |  |
| LSLAN\_SWITCH\_MODEL | Legacy S-LAN Switch Model | String | 100 |  |
| LSLAN\_PORT\_TOTAL | Legacy S-LAN Port Total/Switch | String | 10 |  |
| NSLAN\_USED\_PORTS | Legacy S-LAN Used Ports | Integer | 4 |  |
| NSLAN\_PRESENT | New S-LAN Present | String | 10 |  |
| NSLAN\_SWITCH\_NAME | New S-LAN Switch name | String | 100 |  |
| NSLAN\_SWITCH\_MANUFAC | New S-LAN Switch Manufacturer | String | 50 |  |
| NSLAN\_SWITCH\_MODEL | New S-LAN Switch Model | String | 100 |  |
| NSLAN\_PORT\_TOTAL | New S-LAN Port Total/Switch | String | 10 |  |
| RACK\_AVAIL | Available Rack Units on SLAN Rack | String | 10 |  |
| RACK\_ID | Rack Unit Number/ID | String | 50 |  |
| RACK\_AVAIL\_NUM | Rack Unit Available Quantity | Integer | 4 |  |
| DOOR\_DAISY\_CHAIN | Door Daisy chained | String | 10 |  |
| TECHNICAL\_ISSUE | Technical Issues | String | 100 |  |
| BLACKBOARD\_SPACE | Backboard Space Available to install ACS | String | 10 |  |
| INSTALL\_BLACKBOARD | Install BackBoard | String | 10 |  |
| AVAIL\_OUTLET | Available Dedicated Outlet within 3â€™ of Relay Rack | String | 10 |  |
| AVAIL\_OUTLET\_INSIDE | Available Dedicated Outlets Inside Data Cabinet | String | 10 |  |
| NETWORK\_EQUIPMENT | Network Equipment Power Panel on UPS | String | 10 |  |
| TR\_GROUND\_BAR | TR Ground Bar | String | 10 |  |
| GROUNDED | Relay Racks / Data Cabinet Grounded | String | 10 |  |
| DEDICATED\_AC | Dedicated A/C | String | 10 |  |
| THERMOSTAT | Thermostat | String | 10 |  |
| LIGHTING | Acceptable Lighting Levels | String | 10 |  |
| SECURITY\_CAMERA | Security Camera | String | 10 |  |
| LENEL\_PANEL | Lenel Panel | String | 10 |  |
| MDI\_PANEL | MDI Panel | String | 10 |  |
| CCTV | CCTV Coverage | String | 10 |  |
| CCTV\_TYPE | CCTV Coverage Type | String | 50 |  |
| WORK\_AREA | Work Area Clean | String | 10 |  |
| FLOOR | Floor Clean | String | 10 |  |
| TRASH | Free of Trash | String | 10 |  |
| ROOM\_CONDITION | Room Condition Issues | String | 1000 |  |
| HVAC\_ACCEPT | HVAC Adequate | String | 10 |  |
| SLAN\_ACCEPT | S-LAN Adequate to Support ACS Installation | String | 10 |  |
| POWER\_ACCEPT | Power Adequate to Support ACS Installation | String | 50 |  |
| OTHER | OTHER | String | 1073741822 |  |
| NSLAN\_USED\_PORTS\_1 | New S-LAN Used Ports | Integer | 4 |  |
| FLOOR\_LEVEL | Floor Level | String | 50 |  |
| EP\_SUBPANEL | EP\_SUBPANEL | String | 10 |  |
| EP\_SUBPANEL\_NAME | E-Power SubPanel Names | String | 2000 |  |
| EP\_SPARE\_BREAKER\_NUM | E-Power Number Spare Breakers | String | 50 |  |
| EP\_SPARE\_BLANKS | E-Power Spare Blanks | String | 50 |  |
| PERCENT\_LOAD\_UPS | Percent Load of UPS | String | 50 |  |
| MAX\_LOAD\_UPS | Max Load of UPS | String | 50 |  |
| SSR\_ID | SSR\_ID | String | 16 |  |
| TWC\_ID | TWC ID | String | 15 |  |
| TWC\_ROOM | TWC\_ROOM | String | 16 |  |
| SSR\_ROOM\_NUM | SSR\_ROOM\_NUM | String | 15 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SSR\_ROOMS | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| ROOM\_ID | Room Number | String | 50 |  |
| CONDUCTED\_ON | Conducted On | Date | 8 |  |
| PREPARED\_BY | Prepared By | String | 50 |  |
| ACS\_DOOR\_SRVY | ACS Door Survey Completed | String | 10 | YES\_NO\_OTHER |
| EP\_PRESENT | E-Power Present | String | 10 | YES\_NO\_OTHER |
| EP\_CIRCUIT\_NUM | E-Power Circuit Numbers | String | 100 |  |
| EP\_SPACE\_AVAIL | E-Power Available Space | String | 10 | YES\_NO\_OTHER |
| LSLAN\_PRESENT | Legacy S-LAN Present | String | 10 | YES\_NO\_OTHER |
| LSLAN\_SWITCH\_NAME | Legacy S-LAN Switch Name | String | 100 |  |
| LSLAN\_SWITCH\_MANUFAC | Legacy S-LAN Switch Manufacturer | String | 100 | SSR\_S\_SWITCH\_MAN |
| LSLAN\_SWITCH\_MODEL | Legacy S-LAN Switch Model | String | 100 |  |
| LSLAN\_PORT\_TOTAL | Legacy S-LAN Port Total/Switch | String | 10 | SSR\_SLAN\_PORT |
| NSLAN\_USED\_PORTS | Legacy S-LAN Used Ports | Integer | 4 |  |
| NSLAN\_PRESENT | New S-LAN Present | String | 10 | YES\_NO\_OTHER |
| NSLAN\_SWITCH\_NAME | New S-LAN Switch name | String | 100 |  |
| NSLAN\_SWITCH\_MANUFAC | New S-LAN Switch Manufacturer | String | 50 | SSR\_S\_SWITCH\_MAN |
| NSLAN\_SWITCH\_MODEL | New S-LAN Switch Model | String | 100 |  |
| NSLAN\_PORT\_TOTAL | New S-LAN Port Total/Switch | String | 10 | SSR\_SLAN\_PORT |
| RACK\_AVAIL | Available Rack Units on SLAN Rack | String | 10 | YES\_NO\_OTHER |
| RACK\_ID | Rack Unit Number/ID | String | 50 |  |
| RACK\_AVAIL\_NUM | Rack Unit Available Quantity | Integer | 4 |  |
| DOOR\_DAISY\_CHAIN | Door Daisy chained | String | 10 | YES\_NO\_OTHER |
| TECHNICAL\_ISSUE | Technical Issues | String | 100 |  |
| BLACKBOARD\_SPACE | Backboard Space Available to install ACS | String | 10 | YES\_NO\_OTHER |
| INSTALL\_BLACKBOARD | Install BackBoard | String | 10 | YES\_NO\_OTHER |
| AVAIL\_OUTLET | Available Dedicated Outlet within 3â€™ of Relay Rack | String | 10 | YES\_NO\_OTHER |
| AVAIL\_OUTLET\_INSIDE | Available Dedicated Outlets Inside Data Cabinet | String | 10 | YES\_NO\_OTHER |
| NETWORK\_EQUIPMENT | Network Equipment Power Panel on UPS | String | 10 | YES\_NO\_OTHER |
| TR\_GROUND\_BAR | TR Ground Bar | String | 10 | YES\_NO\_OTHER |
| GROUNDED | Relay Racks / Data Cabinet Grounded | String | 10 | YES\_NO\_OTHER |
| DEDICATED\_AC | Dedicated A/C | String | 10 | YES\_NO\_OTHER |
| THERMOSTAT | Thermostat | String | 10 | YES\_NO\_OTHER |
| LIGHTING | Acceptable Lighting Levels | String | 10 | YES\_NO\_OTHER |
| SECURITY\_CAMERA | Security Camera | String | 10 | YES\_NO\_OTHER |
| LENEL\_PANEL | Lenel Panel | String | 10 | YES\_NO\_OTHER |
| MDI\_PANEL | MDI Panel | String | 10 | YES\_NO\_OTHER |
| CCTV | CCTV Coverage | String | 10 | YES\_NO\_OTHER |
| CCTV\_TYPE | CCTV Coverage Type | String | 50 | PORTAL\_AREA\_TYPE |
| WORK\_AREA | Work Area Clean | String | 10 | YES\_NO\_OTHER |
| FLOOR | Floor Clean | String | 10 | YES\_NO\_OTHER |
| TRASH | Free of Trash | String | 10 | YES\_NO\_OTHER |
| ROOM\_CONDITION | Room Condition Issues | String | 1000 |  |
| HVAC\_ACCEPT | HVAC Adequate | String | 10 | YES\_NO\_OTHER |
| SLAN\_ACCEPT | S-LAN Adequate to Support ACS Installation | String | 10 | YES\_NO\_OTHER |
| POWER\_ACCEPT | Power Adequate to Support ACS Installation | String | 50 |  |
| OTHER | OTHER | String | 1073741822 |  |
| NSLAN\_USED\_PORTS\_1 | New S-LAN Used Ports | Integer | 4 |  |
| FLOOR\_LEVEL | Floor Level | String | 50 | LEVEL |
| EP\_SUBPANEL | EP\_SUBPANEL | String | 10 | YES\_NO\_OTHER |
| EP\_SUBPANEL\_NAME | E-Power SubPanel Names | String | 2000 |  |
| EP\_SPARE\_BREAKER\_NUM | E-Power Number Spare Breakers | String | 50 |  |
| EP\_SPARE\_BLANKS | E-Power Spare Blanks | String | 50 |  |
| PERCENT\_LOAD\_UPS | Percent Load of UPS | String | 50 |  |
| MAX\_LOAD\_UPS | Max Load of UPS | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SSR\_ROOMS\_\_ATTACH | | | | |
| ATTACHMENTID | ATTACHMENTID | OID | 4 |  |
| REL\_OBJECTID | REL\_OBJECTID | Integer | 4 |  |
| CONTENT\_TYPE | CONTENT\_TYPE | String | 150 |  |
| ATT\_NAME | ATT\_NAME | String | 250 |  |
| DATA\_SIZE | DATA\_SIZE | Integer | 4 |  |
| DATA | DATA | Blob | 0 |  |
| STRUCTURES\_SFO | | | | |
| OBJECTID\_1 | OBJECTID\_1 | OID | 4 |  |
| GLOBALID | GLOBALID | GlobalID | 38 |  |
| NAME | NAME | String | 200 |  |
| NUMBER\_ | NUMBER\_ | String | 50 |  |
| DESCRIPTION | DESCRIPTION | String | 1000 |  |
| LABEL | LABEL | String | 100 |  |
| AKA | AKA | String | 100 |  |
| ARCHIVE | ARCHIVE | String | 100 |  |
| OCCUPANT | OCCUPANT | String | 1000 |  |
| TYPE | TYPE | String | 50 |  |
| SQFT | SQFT | Double | 8 |  |
| RETIRED | RETIRED | String | 50 |  |
| STATUS | STATUS | String | 50 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| STRUCTURES\_SFO\_ATTACH | | | | |
| ATTACHMENTID | ATTACHMENTID | OID | 4 |  |
| REL\_GLOBALID | REL\_GLOBALID | GUID | 38 |  |
| CONTENT\_TYPE | CONTENT\_TYPE | String | 150 |  |
| ATT\_NAME | ATT\_NAME | String | 250 |  |
| DATA\_SIZE | DATA\_SIZE | Integer | 4 |  |
| DATA | DATA | Blob | 0 |  |
| GLOBALID | GLOBALID | GlobalID | 38 |  |
| STRUCTURES\_ZONES | | | | |
| OBJECTID\_12 | OBJECTID\_12 | OID | 4 |  |
| OBJECTID\_1 | OBJECTID\_1 | Integer | 4 |  |
| OBJECTID | OBJECTID | Integer | 4 |  |
| GID | GID | Integer | 4 |  |
| NAME | NAME | String | 50 |  |
| DESCRIP | DESCRIP | String | 254 |  |
| STATUS | STATUS | String | 20 |  |
| ALTERNATIV | ALTERNATIV | Integer | 4 |  |
| COMMENTS | COMMENTS | String | 150 |  |
| USERFLAG | USERFLAG | String | 254 |  |
| CADDLAYERN | CADDLAYERN | String | 40 |  |
| CADDLAYERD | CADDLAYERD | String | 50 |  |
| CADDCOLOR | CADDCOLOR | Integer | 4 |  |
| DATEDATAAC | DATEDATAAC | Date | 8 |  |
| DATASOURCE | DATASOURCE | String | 50 |  |
| SHAPE\_LENG | SHAPE\_LENG | Double | 8 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| C\_BLDG\_OTLNAnno | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FEATUREID | FEATUREID | Integer | 4 |  |
| ZORDER | ZORDER | Integer | 4 |  |
| ANNOTATIONCLASSID | ANNOTATIONCLASSID | Integer | 4 |  |
| ELEMENT | ELEMENT | Blob | 0 |  |
| SYMBOLID | SYMBOLID | Integer | 4 |  |
| STATUS | STATUS | SmallInteger | 2 | AnnotationStatus |
| TEXTSTRING | TEXTSTRING | String | 255 |  |
| FONTNAME | FONTNAME | String | 255 |  |
| FONTSIZE | FONTSIZE | Double | 8 |  |
| BOLD | BOLD | SmallInteger | 2 | BooleanSymbolValue |
| ITALIC | ITALIC | SmallInteger | 2 | BooleanSymbolValue |
| UNDERLINE | UNDERLINE | SmallInteger | 2 | BooleanSymbolValue |
| VERTICALALIGNMENT | VERTICALALIGNMENT | SmallInteger | 2 | VerticalAlignment |
| HORIZONTALALIGNMENT | HORIZONTALALIGNMENT | SmallInteger | 2 | HorizontalAlignment |
| XOFFSET | XOFFSET | Double | 8 |  |
| YOFFSET | YOFFSET | Double | 8 |  |
| ANGLE | ANGLE | Double | 8 |  |
| FONTLEADING | FONTLEADING | Double | 8 |  |
| WORDSPACING | WORDSPACING | Double | 8 |  |
| CHARACTERWIDTH | CHARACTERWIDTH | Double | 8 |  |
| CHARACTERSPACING | CHARACTERSPACING | Double | 8 |  |
| FLIPANGLE | FLIPANGLE | Double | 8 |  |
| OVERRIDE | OVERRIDE | Integer | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |
| C\_BLDG\_OTLN\_selectionAnno | | | | |
| OBJECTID | OBJECTID | OID | 4 |  |
| FEATUREID | FEATUREID | Integer | 4 |  |
| ZORDER | ZORDER | Integer | 4 |  |
| ANNOTATIONCLASSID | ANNOTATIONCLASSID | Integer | 4 |  |
| ELEMENT | ELEMENT | Blob | 0 |  |
| SYMBOLID | SYMBOLID | Integer | 4 |  |
| STATUS | STATUS | SmallInteger | 2 | AnnotationStatus |
| TEXTSTRING | TEXTSTRING | String | 255 |  |
| FONTNAME | FONTNAME | String | 255 |  |
| FONTSIZE | FONTSIZE | Double | 8 |  |
| BOLD | BOLD | SmallInteger | 2 | BooleanSymbolValue |
| ITALIC | ITALIC | SmallInteger | 2 | BooleanSymbolValue |
| UNDERLINE | UNDERLINE | SmallInteger | 2 | BooleanSymbolValue |
| VERTICALALIGNMENT | VERTICALALIGNMENT | SmallInteger | 2 | VerticalAlignment |
| HORIZONTALALIGNMENT | HORIZONTALALIGNMENT | SmallInteger | 2 | HorizontalAlignment |
| XOFFSET | XOFFSET | Double | 8 |  |
| YOFFSET | YOFFSET | Double | 8 |  |
| ANGLE | ANGLE | Double | 8 |  |
| FONTLEADING | FONTLEADING | Double | 8 |  |
| WORDSPACING | WORDSPACING | Double | 8 |  |
| CHARACTERWIDTH | CHARACTERWIDTH | Double | 8 |  |
| CHARACTERSPACING | CHARACTERSPACING | Double | 8 |  |
| FLIPANGLE | FLIPANGLE | Double | 8 |  |
| OVERRIDE | OVERRIDE | Integer | 4 |  |
| SHAPE | SHAPE | Geometry | 0 |  |
| SHAPE\_Length | SHAPE\_Length | Double | 8 |  |
| SHAPE\_Area | SHAPE\_Area | Double | 8 |  |

## Domains

|  |  |
| --- | --- |
| Name: YES\_NO\_OTHER |  |
| Description: Yes No Other |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| Yes | Yes |
| No | No |
|  |  |
| Name: SFO\_LEVEL2\_SPACE\_DEMO |  |
| Description: Demo Domain |  |
| Type: esriDTCodedValue |  |
| Code | Description |
|  |  |
| Name: CodeTaxiwayType |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| AIR\_TAXIWAY | AIR\_TAXIWAY |
| AIR\_TLANE | AIR\_TLANE |
| APRON | APRON |
| BYPASS | BYPASS |
| CROSS\_OVER | CROSS\_OVER |
| EAT | EAT |
| ENTER\_EXIT\_TAXIWAY | ENTER\_EXIT\_TAXIWAY |
| EXIT | EXIT |
| FASTEXIT | FASTEXIT |
| GATE\_TLANE | GATE\_TLANE |
| GND | GND |
| HOLDING | HOLDING |
| INLINE | INLINE |
| OTHER | OTHER |
| PARALLEL | PARALLEL |
| STUB | STUB |
| TLANE | TLANE |
|  |  |
| Name: CodeOwner |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| A | A |
| B | B |
| C | C |
| E | E |
| F | F |
| H | H |
| I | I |
| J | J |
| K | K |
| L | L |
| N | N |
| O | O |
| P | P |
| R | R |
| S | S |
|  |  |
| Name: PORTAL\_AREA\_TYPE |  |
| Description: Area Types Portal Leads to and From |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| Secure | Secure |
| Sterile | Sterile |
| Public | Public |
| Other | Other |
|  |  |
| Name: CodeLightingConfigurationType |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| ALSF-1 | ALSF-1 |
| ALSF-2 | ALSF-2 |
| APAP | APAP |
| APBN | APBN |
| CLRBAR | CLRBAR |
| CODEBEACON | CODEBEACON |
| COURSE | COURSE |
| F | F |
| FL | FL |
| FL (2) | FL (2) |
| FL (2+1) | FL (2+1) |
| HLL | HLL |
| HLLL | HLLL |
| HPIL | HPIL |
| HPPEL | HPPEL |
| HPPLSF | HPPLSF |
| ISO | ISO |
| L-804 | L-804 |
| L-850A | L-850A |
| L-850B | L-850B |
| L-850C | L-850C |
| L-850D | L-850D |
| L-850E | L-850E |
| L-850F | L-850F |
| L-852A | L-852A |
| L-852B | L-852B |
| L-852C | L-852C |
| L-852D | L-852D |
| L-852E | L-852E |
| L-852E/F | L-852E/F |
| L-852F | L-852F |
| L-852G | L-852G |
| L-852G/S | L-852G/S |
| L-852J | L-852J |
| L-852K | L-852K |
| L-852S | L-852S |
| L-852T | L-852T |
| L-853 | L-853 |
| L-854 | L-854 |
| L-860 | L-860 |
| L-860E | L-860E |
| L-861 | L-861 |
| L-861E | L-861E |
| L-861SE | L-861SE |
| L-861T | L-861T |
| L-862 | L-862 |
| L-862E | L-862E |
| L-862S | L-862S |
| L-880/L881 | L-880/L881 |
| LDIN | LDIN |
| MALS | MALS |
| MALSF | MALSF |
| MALSR | MALSR |
| MO (A) | MO (A) |
| NONE | NONE |
| OBSCAT | OBSCAT |
| OBSDUAL | OBSDUAL |
| OBSRED | OBSRED |
| OBSWHITE | OBSWHITE |
| OC | OC |
| ODALS | ODALS |
| OTHER | OTHER |
| PAPI2 | PAPI2 |
| PAPI4 | PAPI4 |
| PORTABLE | PORTABLE |
| PVASI | PVASI |
| Q | Q |
| RAIL | RAIL |
| REIL | REIL |
| RWSL | RWSL |
| SALS | SALS |
| SMGCS | SMGCS |
| SSALF | SSALF |
| SSALR | SSALR |
| TRCV | TRCV |
| T-VASI | T-VASI |
| TWYON\_OFFLGT | TWYON\_OFFLGT |
| VASI-12 | VASI-12 |
| VASI-16 | VASI-16 |
| VASI-2 | VASI-2 |
| VASI-2-2 | VASI-2-2 |
|  |  |
| Name: CodeDirectionality |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| BI | BI |
| ES | ES |
|  |  |
| Name: CodeColor |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| AMBER | AMBER |
| BLACK | BLACK |
| BLUE | BLUE |
| BROWN | BROWN |
| GREEN | GREEN |
| GREEN-GREEN | GREEN-GREEN |
| GREEN-RED | GREEN-RED |
| GREEN-YELLOW | GREEN-YELLOW |
| GREY | GREY |
| LIGHTGREY | LIGHTGREY |
| MAGENTA | MAGENTA |
| ORANGE | ORANGE |
| OTHER | OTHER |
| PINK | PINK |
| PURPLE | PURPLE |
| RED | RED |
| RED-GREEN | RED-GREEN |
| RED-RED | RED-RED |
| TBD | TBD |
| VIOLET | VIOLET |
| WHITE | WHITE |
| WHITE-RED | WHITE-RED |
| WHITE-WHITE | WHITE-WHITE |
| WHITE-YELLOW | WHITE-YELLOW |
| YELLOW | YELLOW |
| YELLOW-GREEN | YELLOW-GREEN |
| YELLOW-RED | YELLOW-RED |
|  |  |
| Name: CodeDesignGroup |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| I | I |
| II | II |
| III | III |
| IV | IV |
| V | V |
|  |  |
| Name: CodeGateStandType |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| ANG-NI | ANG-NI |
| ANG-NO | ANG-NO |
| HS | HS |
| ISO | ISO |
| JB | JB |
| NI | NI |
| OTHER | OTHER |
| PR | PR |
| RMT | RMT |
| SR | SR |
| TM | TM |
|  |  |
| Name: PLAN\_OEAAA\_ON\_STRUCTYPE |  |
| Description: Planning OEAAA On structure type |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| Building | Building |
| Equipment | Equipment |
| Other | Other |
| Runway | Runway |
| Taxiway | Taxiway |
| Crane (Temporary) | Crane (Temporary) |
|  |  |
| Name: CodeMarkingFeatureType |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| AIMING\_POINT | AIMING\_POINT |
| ALTBAND | ALTBAND |
| APRON\_SIGN | APRON\_SIGN |
| ARROW | ARROW |
| ARROW\_HEAD | ARROW\_HEAD |
| CHECKERBOARD | CHECKERBOARD |
| CHEVRON | CHEVRON |
| DEMARCATION | DEMARCATION |
| DIR\_SIGN | DIR\_SIGN |
| GATE\_LINE | GATE\_LINE |
| GATE\_SIGN | GATE\_SIGN |
| HOLD\_SIGN | HOLD\_SIGN |
| ILS\_HOLD | ILS\_HOLD |
| INTERSECTION\_HOLD | INTERSECTION\_HOLD |
| LAHSO | LAHSO |
| LOCATION\_SIGN | LOCATION\_SIGN |
| NON\_MOVE\_AREA | NON\_MOVE\_AREA |
| NONE | NONE |
| OTHER | OTHER |
| OTHER\_LINE | OTHER\_LINE |
| OTHER\_POLYGON | OTHER\_POLYGON |
| PERM\_CLOSED | PERM\_CLOSED |
| POS\_SIGN | POS\_SIGN |
| RWY\_CL | RWY\_CL |
| RWY\_HOLD | RWY\_HOLD |
| RWY\_ID | RWY\_ID |
| RWY\_SHD | RWY\_SHD |
| RWY\_THRSH | RWY\_THRSH |
| SIDE\_STRP | SIDE\_STRP |
| SOLID | SOLID |
| TDZ\_MARK | TDZ\_MARK |
| TEMP\_CLOSED | TEMP\_CLOSED |
| THRSH\_BAR | THRSH\_BAR |
| TIEDOWN | TIEDOWN |
| TWY\_CL | TWY\_CL |
| TWY\_EDGE | TWY\_EDGE |
| TWY\_HOLD | TWY\_HOLD |
| TWY\_SHD | TWY\_SHD |
|  |  |
| Name: CodeSurfaceType |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| P | P |
| S | S |
|  |  |
| Name: FLOOR\_LEVEL |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| 1 | 1 |
| 2 | 2 |
| 3 | 3 |
| 4 | 4 |
| 5 | 5 |
| 6 | 6 |
| 7 | 7 |
| 8 | 8 |
| Basement | Basement |
| Mezzanine | Mezzanine |
|  |  |
| Name: SSR\_SLAN\_PORT |  |
| Description: SSR SLAN Port Count |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| 0 | 0 |
| 8 | 8 |
| 16 | 16 |
| 24 | 24 |
| 32 | 32 |
| 40 | 40 |
| 48 | 48 |
| Other | Other |
| 96 | 96 |
| 128 | 128 |
| 240 | 240 |
| 384 | 384 |
|  |  |
| Name: CodeLoadingBridgeType |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| ARM | ARM |
| OTHER | OTHER |
| PORTABLE\_RAMP | PORTABLE\_RAMP |
|  |  |
| Name: AnnotationStatus |  |
| Description: Valid annotation state values. |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| Placed | 0 |
|  |  |
| Name: SSR\_S\_SWITCH\_MAN |  |
| Description: SSR Switch Manufacturer |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| Juniper | Juniper |
| Cisco | Cisco |
|  |  |
| Name: CodeBoolean |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| N | N |
|  |  |
| Name: CodeVerticalStructureMaterial |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| COMPOSITION | COMPOSITION |
| CONCRETE | CONCRETE |
| METAL | METAL |
| ROCK | ROCK |
| STONE\_BRICK | STONE\_BRICK |
|  |  |
| Name: CodeSegmentType |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| BEGIN | BEGIN |
| CONNECTING | CONNECTING |
| END | END |
|  |  |
| Name: CodeSurfaceCondition |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| FAIR | FAIR |
| GOOD | GOOD |
| OTHER | OTHER |
| POOR | POOR |
|  |  |
| Name: CodeStatus |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| ABANDONED | ABANDONED |
| ACTIVE | ACTIVE |
| AIRSPACED | AIRSPACED |
| AS\_BUILT | AS\_BUILT |
| BROKEN | BROKEN |
| CLOSED | CLOSED |
| CONDEMNED | CONDEMNED |
| DEMOLISHED | DEMOLISHED |
| ENV\_CLEARED | ENV\_CLEARED |
| FAILED\_AID | FAILED\_AID |
| INACTIVE | INACTIVE |
| LIMITED | LIMITED |
| LONG\_TERM | LONG\_TERM |
| MEDIUM\_TERM | MEDIUM\_TERM |
| NON\_OPERATIONAL | NON\_OPERATIONAL |
| OCCUPIED | OCCUPIED |
| OPERATIONAL | OPERATIONAL |
| OTHER | OTHER |
| PARKED | PARKED |
| PERMANENT | PERMANENT |
| PORTABLE | PORTABLE |
| RELEASED | RELEASED |
| S\_POWER | S\_POWER |
| SEMI\_PERMANENT | SEMI\_PERMANENT |
| SHORT\_TERM | SHORT\_TERM |
| TBD | TBD |
| TEMPORARY | TEMPORARY |
| TERMINATED | TERMINATED |
| UNDER\_CONSTRUCTION | UNDER\_CONSTRUCTION |
| UNKNOWN | UNKNOWN |
| UNOCCUPIED | UNOCCUPIED |
|  |  |
| Name: LEVEL |  |
| Description: LEVEL |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| 1 | 1 |
| 2 | 2 |
| 3 | 3 |
| 4 | 4 |
| 5 | 5 |
| 6 | 6 |
| 7 | 7 |
| 8 | 8 |
| 9 | 9 |
| Basement | Basement |
| Roof | Roof |
| Other | 0 |
|  |  |
| Name: VerticalAlignment |  |
| Description: Valid symbol vertical alignment values. |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| Top | 0 |
| Center | 1 |
| Baseline | 2 |
|  |  |
| Name: CodeBridgeType |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| ROAD | ROAD |
| RR | RR |
| RWY | RWY |
|  |  |
| Name: PLAN\_OEAAA\_OFF\_STRUCTYPE |  |
| Description: Planning OEAAA Off structure type |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| Antenna (Side Mount) | Antenna (Side Mount) |
| Antenna (Top Mount) | Antenna (Top Mount) |
| Antenna (Tower) | Antenna (Tower) |
| Building | Building |
| Crane | Crane |
| Lighting Study | Lighting Study |
| Other (w/Antenna) | Other (w/Antenna) |
| Other (w/o Antenna) | Other (w/o Antenna) |
| Tower | Tower |
|  |  |
| Name: CodeSurfaceMaterial |  |
| Description: |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| AG | AG |
| Ags | Ags |
| ANG | ANG |
| BE | BE |
| CA | CA |
| CG | CG |
| CGS | CGS |
| CNG | CNG |
| DS | DS |
| DT | DT |
| EMAS | EMAS |
| FW | FW |
| GR | GR |
| GS | GS |
| SI | SI |
| SW | SW |
|  |  |
| Name: FLOOR\_TYPE |  |
| Description: Arrivals Departures |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| Arrivals | Arrivals |
| Departures | Departures |
| Mezzanine | Mezzanine |
|  |  |
| Name: HorizontalAlignment |  |
| Description: Valid horizontal symbol alignment values. |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| Left | 0 |
| Center | 1 |
| Right | 2 |
|  |  |
| Name: BooleanSymbolValue |  |
| Description: Valid values are Yes and No. |  |
| Type: esriDTCodedValue |  |
| Code | Description |
| Yes | 1 |