## Coordinate System Alignment 

The Airport employs a local coordinate system, SFO-B. Models and drawings submitted to the Airport shall reference the SFO-B coordinate system (x, y, and z coordinates). For more information and instructions on setting up the coordinate system in Revit, see the SFO BIM Guide – Appendix D.